**STEINEL Professional Multisensor**

**Multisensor Aerosol KNX**

**V3.0**

Dimensions (L x W x H): 33 x 123 x 123 mm; With motion detector: No; Manufacturer's Warranty: 5 years; Settings via: ETS software, Bluetooth, Bus; With remote control: No; PU1, EAN: 4007841079192; Type: Other; Application, place: Indoors; Application, room: classroom, lecture hall, one-person office, recreation room, duty room, conference room / meeting room, Indoors, kitchenette; Colour: white; Colour, RAL: 9003; Includes corner wall mount: No; Installation site: ceiling; Installation: Concealed wiring, Ceiling; IP-rating: IP20; Ambient temperature: from 0 up to 40 °C; Material: Plastic; Mains power supply: 30 V; Power consumption: 0,5 W; Power supply, detail: KNX bus; With bus coupling: Yes; Technology, sensors: CO2, Photo-cell controller, Air pressure, Air humidity, Temperature, VOC; Optimum mounting height: 2,8 m; Twilight setting: 2 – 1000 lx; Twilight setting TEACH: Yes; Constant-lighting control: No; KNX functions: Risk of infection, Udes air, Comfort, CO2, Light level, HVAC output, Logic gate, Air pressure, Humidity output, Day / night function, Dewpoint, Temperature output, VOC; Interconnection: Yes; Interconnection via: KNX bus; Rated current: 15 mA; Product category: Multisensor

**Manufacturer** Steinel

**Prod. No.** 079192

**Ordering designation** Multisensor Aerosol KNX

Deliver, install and set ready for operation