**STEINEL Professional Presence detector**

**Hallway**

**DALI-2 Input Device - concealed**

Dimensions (L x W x H): 67 x 103 x 103 mm; With motion detector: Yes; Manufacturer's Warranty: 5 years; Settings via: Bluetooth, Bus; With remote control: No; Version: DALI-2 Input Device - concealed; PU1, EAN: 4007841064532; Type: Presence detector; Application, place: Indoors; Application, room: Indoors, corridor / aisle; Colour: white; Colour, RAL: 9003; Includes corner wall mount: No; Installation site: ceiling; Installation: Concealed wiring, Ceiling; IP-rating: IP20; Ambient temperature: from -20 up to 50 °C; Material: Plastic; Mains power supply: 12 – 23 V; Power supply, detail: DALI bus; Steuerausgang, Dali: Addressable/slave; With bus coupling: Yes; Technology, sensors: High frequency, Light sensor, Temperature, Air humidity; Mounting height: 2,00 – 4,00 m; Mounting height max.: 4,00 m; Optimum mounting height: 2,8 m; HF-system: 5,8 GHz; Detection: also through glass, wood and stud walls; Detection angle: Aisle, 360 °; Angle of aperture: 140 °; Sneak-by guard: Yes; Capability of masking out individual segments: No; Electronic scalability: Yes; Mechanical scalability: No; Reach, radial: 25 x 3 m (75 m²); Reach, tangential: 25 x 3 m (75 m²); Transmitter power: < 1 mW; Basic light level function: No; Main light adjustable: No; Twilight setting TEACH: No; Constant-lighting control: No; Interconnection: Yes; Type of interconnection: Master/slave; Interconnection via: Bluetooth, DALI bus; Product category: Presence detector

**Manufacturer** Steinel

**Prod. No.** 064532

**Ordering designation** Hallway DALI-2 Input Device - concealed

Deliver, install and set ready for operation