**STEINEL Professional Presence detector**

**Hallway**

**IP - concealed**

Dimensions (L x W x H): 68 x 103 x 103 mm; With motion detector: Yes; Manufacturer's Warranty: 5 years; Settings via: Bluetooth, Web-Interface; With remote control: No; Version: IP - concealed; PU1, EAN: 4007841066161; Type: Presence detector; Application, place: Indoors; Application, room: Indoors, corridor / aisle; Colour: white; Colour, RAL: 9003; Includes corner wall mount: No; Installation site: ceiling; Installation: Concealed wiring, Ceiling; IP-rating: IP20; Ambient temperature: from -20 up to 50 °C; Material: Plastic; Mains power supply: 18 – 55 V; Power supply, detail: Passive PoE SELV, standard PoE (IEEE 802.3 af); Technology, sensors: High frequency, Light sensor, Temperature, Air humidity; Mounting height: 2,00 – 4,00 m; Mounting height max.: 4,00 m; Optimum mounting height: 2,8 m; HF-system: 5,8 GHz; Detection: also through glass, wood and stud walls; Detection angle: Aisle, 360 °; Angle of aperture: 140 °; Sneak-by guard: Yes; Capability of masking out individual segments: No; Electronic scalability: Yes; Mechanical scalability: No; Reach, radial: 25 x 3 m (75 m²); Reach, tangential: 25 x 3 m (75 m²); Transmitter power: < 1 mW; Basic light level function: No; Main light adjustable: No; Twilight setting TEACH: No; Constant-lighting control: No; Interconnection: Yes; Interconnection via: Bluetooth, LAN; Product category: Presence detector

**Manufacturer** Steinel

**Prod. No.** 066161

**Ordering designation** Hallway IP - concealed

Deliver, install and set ready for operation