**STEINEL Professional Motion detector**

**IS 2360-3 ECO 24m**

**black**

Dimensions (Ø x H): 121 x 57 mm; With motion detector: Yes; Manufacturer's Warranty: 5 years; Settings via: Potentiometers; With remote control: No; Version: black; PU1, EAN: 4007841081706; Type: Motion detectors; Application, place: Outdoors, Indoors; Application, room: corridor / aisle, changing room, function room / ancillary room, kitchenette, stairwell, WC / washroom, multi-storey / underground car park, outdoors, warehouse, Indoors; Colour: black; Colour, RAL: 9005; Includes corner wall mount: No; Installation site: ceiling; Installation: Surface wiring, Ceiling; IP-rating: IP54; Protection class: II; Ambient temperature: from -20 up to 50 °C; Material: Plastic; Mains power supply: 220 – 240 V / 50 – 60 Hz; Switching output 1, resistive: 2000 W; Switching output 1, number of LEDs / fluorescent lamps: 8 pcs.; Switching output 1, floating: No; Fluorescent lamps, electronic ballast: 500 W; Fluorescent lamps, series-corrected: 900 VA; Fluorescent lamps, parallel-corrected: 400 VA; Switching output 1, low-voltage halogen lamps: 1000 VA; LED lamps < 2 W: 100 W; LED lamps > 2 W < 8 W: 250 W; LED lamps > 8 W: 500 W; Capacitive load in μF: 176 µF; Power consumption: 0,56 W; Technology, sensors: passive infrared, Light sensor; Mounting height: 2,50 – 6,00 m; Mounting height max.: 6,00 m; Optimum mounting height: 2,8 m; Detection angle: 360 °; Angle of aperture: 90 °; Sneak-by guard: Yes; Capability of masking out individual segments: Yes; Electronic scalability: No; Mechanical scalability: No; Reach, radial: Ø 6 m (28 m²); Reach, tangential: Ø 24 m (452 m²); Switching zones: 972 switching zones; Cover material: shrouds; Twilight setting: 2 – 1000 lx; Time setting: 5 sec – 15 min; Basic light level function: No; Main light adjustable: No; Twilight setting TEACH: No; Constant-lighting control: No; Interconnection: Yes; Type of interconnection: Master/master; Interconnection via: Cable; Interconnection, number: max 5 sensors; Product category: Motion detector

**Manufacturer** Steinel

**Prod. No.** 081706

**Ordering designation** IS 2360-3 ECO 24m black

Deliver, install and set ready for operation