**STEINEL Professional Presence detector**

**US 360**

**DALI-2 Input Device**

Dimensions (L x W x H): 67 x 120 x 120 mm; With motion detector: Yes; Manufacturer's Warranty: 5 years; Settings via: Bus; With remote control: No; Version: DALI-2 Input Device; PU1, EAN: 4007841057534; Type: Presence detector; Application, place: Indoors; Application, room: classroom, one-person office, open-plan office, conference room / meeting room, duty room, recreation room, function room / ancillary room, stairwell, WC / washroom, Indoors; Colour: white; Colour, RAL: 9010; Includes corner wall mount: No; Installation site: ceiling; Installation: Concealed wiring, Ceiling; IP-rating: IP20; Ambient temperature: from -25 up to 55 °C; Material: Plastic; Mains power supply: 16 V; Power supply, detail: DALI bus; Number of Dali users: 12; Steuerausgang, Dali: Addressable/slave; With bus coupling: Yes; Technology, sensors: Ultrasonic, Light sensor; Mounting height: 2,50 – 3,5 m; Mounting height max.: 3,50 m; Optimum mounting height: 2,5 m; Ultrasonic technology: 40 kHz; Detection angle: 360 °; Angle of aperture: 180 °; Sneak-by guard: Yes; Capability of masking out individual segments: No; Electronic scalability: Yes; Mechanical scalability: No; Reach, radial: Ø 10 m (79 m²); Reach, tangential: Ø 6 m (28 m²); Reach, presence: Ø 6 m (28 m²); Twilight setting: 10 – 1000 lx; Basic light level function: No; Main light adjustable: No; Twilight setting TEACH: No; Constant-lighting control: No; Interconnection: Yes; Type of interconnection: Master/slave; Interconnection via: DALI bus; Max. Current consumption according to IEC 62386-101: 42 mA; Typical current consumption at 16V input voltage: 16 mA; Max. Current consumption at 10V input voltage in regular operation: 24 mA; Product category: Presence detector

**Manufacturer** Steinel

**Prod. No.** 057534

**Ordering designation** US 360 DALI-2 Input Device

Deliver, install and set ready for operation