**STEINEL Professional Presence detector**

**IR Quattro MICRO 6m**

**KNX - black V3**

Dimensions (Ø x H): 43 x 71 mm; With motion detector: Yes; Manufacturer's Warranty: 5 years; Settings via: ETS software, Remote control, Bus, Smart Remote; With remote control: No; Version: KNX - black; PU1, EAN: 4007841068646; Type: Presence detector; Application, place: Indoors; Application, room: one-person office, hotel room, care room, function room / ancillary room, WC / washroom, Indoors; Colour: black; Colour, RAL: 9005; Includes corner wall mount: No; Installation site: ceiling; Installation: In-ceiling installation, Ceiling; IP-rating: IP65; Ambient temperature: from -25 up to 55 °C; Material: Plastic; Mains power supply: 30 V; Power consumption: 0,5 W; With bus coupling: Yes; Technology, sensors: Photo-cell controller, passive infrared; Mounting height: 2,00 – 5,00 m; Mounting height max.: 5,00 m; Optimum mounting height: 2,8 m; Detection angle: 360 °; Angle of aperture: 90 °; Sneak-by guard: Yes; Capability of masking out individual segments: No; Electronic scalability: No; Mechanical scalability: No; Reach, radial: 4 x 4 m (16 m²); Reach, tangential: 6 x 6 m (36 m²); Reach, presence: 4 x 4 m (16 m²); Switching zones: 168 switching zones; Twilight setting: 2 – 1000 lx; Time setting: 60 sec – 255 min; Basic light level function: Yes; Main light adjustable: 0 - 100 %; Twilight setting TEACH: Yes; Constant-lighting control: Yes; KNX functions: Photo-cell controller, Basic light level function, Light level, HVAC output, Constant-lighting control, Day / night function, Presence output, Light output 4x, Logic gate; Interconnection: Yes; Type of interconnection: Master/master, Master/slave; Interconnection via: KNX bus; Rated current: 10 mA; Product category: Presence detector

**Manufacturer** Steinel

**Prod. No.** 068646

**Ordering designation** IR Quattro MICRO 6m KNX - black

Deliver, install and set ready for operation