**STEINEL Professional Sensor-switched indoor light**

**warm white V2**

Dimensions (Ø x H): 280 x 110 mm; Mains power supply: 220 – 240 V / 50 – 60 Hz; Sensor Technology: High frequency; Output: 9,5 W; Interconnection: Yes; Luminous flux: 960 lm; Colour temperature: 3000 K; Colour Rendering Index: 80-89; With lamp: Yes, STEINEL LED system; Lamp: LED cannot be replaced; LED life expectancy (max. °C): 50000 h; Drop in luminous flux in accordance with LM80: L80B10; Base: without; LED cooling system: Passive Thermo Control; With motion detector: Yes; Detection angle: 360 °; Electronic scalability: Yes; Mechanical scalability: No; Continuous light: selectable, 4h; Twilight setting: 2 – 2000 lx; Time setting: 5 sec – 15 min; Basic light level function: Yes; Basic light level function time: 10/30 min, all night; Soft light start: Yes; Impact resistance: IK03; IP-rating: IP54; Protection class: II; Ambient temperature: -10 – 40 °C; Housing material: Plastic; Cover material: Plastic, opal; Manufacturer's Warranty: 5 years; Version: warm white

**Manufacturer** Steinel

**Prod. No.**

**Ordering designation**

Deliver, install and set ready for operation