**STEINEL Professional LED floodlight without sensor**

**XLED PRO 240 M**

**Anthracite V2**

Dimensions (L x W x H): 161 x 180 x 199 mm; Mains power supply: 220 – 240 V / 50 – 60 Hz; Output: 19,3 W; Interconnection: No; Luminous flux: 2124 lm; Colour temperature: 3000 K; Colour variation LED: SDCM3; With lamp: Yes, STEINEL LED system; Lamp: LED cannot be replaced; LED life expectancy (25 °C): > 60000 h; LED cooling system: HCMC (High Conductive Magnesium Composite); With motion detector: No; Basic light level function: No; Main light adjustable: No; Soft light start: No; Impact resistance: IK03; IP-rating: IP44; Protection class: II; Ambient temperature: -20 – 40 °C; Housing material: HCMC; Cover material: Plastic, opal; Manufacturer's Warranty: 5 years; Includes corner wall mount: Yes; PU1, net weight: 0,64 kg; Version: Anthracite

**Manufacturer** Steinel

**Prod. No.** 068080

**Ordering designation** XLED PRO 240 M Anthracite

Deliver, install and set ready for operation