**STEINEL Professional Bewegingsmelder**

**IS 345**

**KNX - inbouw vierkant zwart V3**

Dimensions (L x W x H): 78 x 94 x 94 mm; Manufacturer's Warranty: 5 jaar; Settings via: ETS-software, Afstandsbediening, Bus, Smart Remote; With remote control: Nee; Version: KNX - inbouw vierkant zwart; PU1, EAN: 4007841084141; Type: Bewegingsmelder; Application, place: Binnen; Application, room: hal / gang, parkeergarage, Binnen; Colour: zwart; Colour, RAL: 9005; Includes corner wall mount: Nee; Installation site: plafond; Installation: In de muur, Plafond; IP-rating: IP20; Ambient temperature: van -20 tot 50 °C; Materiaal: kunststof; Power supply, detail: KNX-bus; With bus coupling: Ja; Mounting height: 2,50 – 5,00 m; Mounting height max.: 5,00 m; Optimum mounting height: 2,5 m; Detection angle: Gang, 360 °; Angle of aperture: 45 °; Sneak-by guard: Ja; Capability of masking out individual segments: Ja; Electronic scalability: Nee; Mechanical scalability: Nee; Reach, radial: 12 x 6 m (72 m²); Reach, tangential: 23 x 6 m (138 m²); Switching zones: 280 schakelzones; Twilight setting: 2 – 1000 lx; Time setting: 5 sec. – 15 min; Basic light level function: Ja; Main light adjustable: 0 - 100 %; Twilight setting TEACH: Ja; Constant-lighting control: Ja; KNX functions: Schemerschakelaar, basislichtfunctie, Lichtsterktewaarde, HVAC-uitgang, Regeling constant licht, Lichtuitgang 2x, Aanwezigheid-uitgang, Dag- / nachtfunctie, Logische poort; Interconnection: Ja; Type of interconnection: Master/slave; Interconnection via: KNX-bus; Rated current: 12,5 mA; Product category: Bewegingsmelder

**Fabrikant** Steinel

**art.nr.** 084141

**Bestelaanduiding** IS 345 KNX - inbouw vierkant zwart

Leveren, monteren en bedrijfsklaar instellen