STEINEL Professional Presence detector

HF 360
KNX - concealed black V3

Dimensions (L x W x H): 55 x 120 x 120 mm;With motion detector: Yes;Manufacturer's Warranty: 5 years;Settings via: ETS software, Remote control, Bus, Smart Remote;With remote control: No;Version: KNX - concealed black;PU1, EAN: 4007841082277;Type: Presence detector;Application, place: Indoors;Application, room: function room / ancillary room, kitchenette, stairwell, WC / washroom, Indoors;Colour: black;Colour, RAL: 9005;Includes corner wall mount: No;Installation site: ceiling;Package content: 1;Installation: Concealed wiring, Ceiling;IP-rating: IP20;Ambient temperature: from -25 up to 55 °C;Material: Plastic;Mains power supply: 30 V;Power consumption: 0,7 W;Power supply, detail: KNX bus;With bus coupling: Yes;Technology, sensors: High frequency, Light sensor;Mounting height: 2,50 – 3,5 m;Mounting height max.: 3,50 m;Optimum mounting height: 2,8 m;HF-system: 5,8 GHz;Detection: also through glass, wood and stud walls;Detection angle: 360 °;Angle of aperture: 140 °;Sneak-by guard: Yes;Capability of masking out individual segments: Yes;Electronic scalability: Yes;Mechanical scalability: No;Reach, radial: Ø 12 m (113 m²);Reach, tangential: Ø 12 m (113 m²);Cover material: sticker;Transmitter power: < 1 mW;Twilight setting: 10 – 1000 lx;Time setting: 10 sec – 1092 min;Basic light level function: Yes;Basic light level function time: 1-255 min;Main light adjustable: 0 - 100 %;Twilight setting TEACH: Yes;Constant-lighting control: Yes;KNX functions: Photo-cell controller, Basic light level function, Light level, HVAC output, Constant-lighting control, Light output 4x, Presence output, Day / night function, Logic gate;Interconnection: Yes;Type of interconnection: Master/master, Master/slave;Interconnection via: KNX bus;Rated current: 30 mA;KNX Medium: TP 256;KNX Secure: No;Product category: Presence detector

Manufacturer Steinel
Prod. No. 082277
Ordering designation HF 360 KNX - concealed black

Deliver, install and set ready for operation
