**STEINEL Professional Rilevatore di presenza**

**Hallway**

**KNX - Sopra intonaco nero V3.5**

Dimensions (L x W x H): 62 x 123 x 123 mm; With motion detector: Sì; Manufacturer's Warranty: 5 anni; Settings via: Bluetooth; With remote control: No; Version: KNX - Sopra intonaco nero; PU1, EAN: 4007841082062; Type: Rilevatore di presenza; Application, place: Interni; Application, room: Interni, corridoio / pianerottolo; Colour: nero; Colour, RAL: 9005; Includes corner wall mount: No; Installation site: soffitto; Installation: In superficie; IP-rating: IP20; Ambient temperature: da -25 fino a 50 °C; Materiale: Plastica; Mains power supply: 30 V; Power consumption: 0,7 W; Power supply, detail: KNX-bus; With bus coupling: Sì; Technology, sensors: Alta frequenza, Sensore ottico; Mounting height: 2 – 4 m; Mounting height max.: 4,00 m; Optimum mounting height: 2,8 m; HF-system: 5,8 GHz; Detection: anche attraverso vetro, legno e pareti in materiale leggero; Detection angle: 360 °; Angle of aperture: 140 °; Sneak-by guard: Sì; Capability of masking out individual segments: No; Electronic scalability: Sì; Mechanical scalability: No; Reach, radial: 25 x 3 m (75 m²); Reach, tangential: 25 x 3 m (75 m²); Transmitter power: < 1 mW; Time setting: 10 sec – 1092 min; Basic light level function: Sì; Main light adjustable: 0 - 100 %; Twilight setting TEACH: Sì; KNX functions: Comodità, Valutazione dei singoli pirosensori, Funzione luce di base, Uscita HVAC, Uscita luce 4x, Uscita presenza, Funzione giorno / funzione notte, Punto di rugiada, Porta logica, Uscita umidità dell'aria, Uscita temperatura; Interconnection: Sì; Type of interconnection: master/master, Master/Slave; Interconnection via: bus KNX; Rated current: 30 mA; Product category: Rilevatore di presenza

**Produttore** Steinel

**Art. n.** 082062

**Denominazione ordine** Hallway KNX - Sopra intonaco nero

Consegnare, montare e impostare in modo che sia pronto alla messa in funzione