**STEINEL Professional Presence detector**

**Hallway**

**KNX - concealed black V3.5**

Dimensions (L x W x H): 67 x 103 x 103 mm; With motion detector: Yes; Manufacturer's Warranty: 5 years; Settings via: Bluetooth; With remote control: No; Version: KNX - concealed black; PU1, EAN: 4007841082079; Type: Presence detector; Application, place: Indoors; Application, room: Indoors, corridor / aisle; Colour: black; Colour, RAL: 9005; Includes corner wall mount: No; Installation site: ceiling; Installation: Concealed wiring; IP-rating: IP20; Ambient temperature: from -25 up to 50 °C; Material: Plastic; Mains power supply: 30 V; Power consumption: 0,7 W; Power supply, detail: KNX bus; With bus coupling: Yes; Technology, sensors: High frequency, Light sensor; Mounting height: 2 – 4 m; Mounting height max.: 4,00 m; Optimum mounting height: 2,8 m; HF-system: 5,8 GHz; Detection: also through glass, wood and stud walls; Detection angle: 360 °; Angle of aperture: 140 °; Sneak-by guard: Yes; Capability of masking out individual segments: No; Electronic scalability: Yes; Mechanical scalability: No; Reach, radial: 25 x 3 m (75 m²); Reach, tangential: 25 x 3 m (75 m²); Transmitter power: < 1 mW; Time setting: 10 sec – 1092 min; Basic light level function: Yes; Main light adjustable: 0 - 100 %; Twilight setting TEACH: Yes; KNX functions: Comfort, Individual pyro evaluation, Basic light level function, HVAC output, Light output 4x, Presence output, Day / night function, Dewpoint, Logic gate, Humidity output, Temperature output; Interconnection: Yes; Type of interconnection: Master/master, Master/slave; Interconnection via: KNX bus; Rated current: 30 mA; Product category: Presence detector

**Manufacturer** Steinel

**Prod. No.** 082079

**Ordering designation** Hallway KNX - concealed black

Deliver, install and set ready for operation