**STEINEL Professional Presence detector**

**HF 360**

**COM1 - in-ceiling installation**

Dimensions (L x W x H): 94 x 120 x 120 mm; Manufacturer's Warranty: 5 years; Settings via: Remote control, DIP switches, Potentiometers, Smart Remote; With remote control: No; Version: COM1 - in-ceiling installation; PU1, EAN: 4007841079512; Type: Presence detector; Application, place: Indoors; Application, room: function room / ancillary room, kitchenette, stairwell, WC / washroom, Indoors; Colour: white; Colour, RAL: 9010; Includes corner wall mount: No; Installation site: ceiling; Installation: In-ceiling installation, Ceiling; IP-rating: IP20; Ambient temperature: -25 – 55 °C; Material: Plastic; Mains power supply: 230 V / 50 – 60 Hz; Technology, sensors: High frequency, Light sensor; Mounting height: 2,50 – 3,50 m; Mounting height max.: 3,50 m; Optimum mounting height: 2,8 m; HF-system: 5,8 GHz; Detection: also through glass, wood and stud walls; Detection angle: 360 °; Angle of aperture: 140 °; Sneak-by guard: Yes; Capability of masking out individual segments: Yes; Electronic scalability: Yes; Mechanical scalability: No; Reach, radial: Ø 12 m (113 m²); Reach, tangential: Ø 12 m (113 m²); Transmitter power: < 1 mW; Functions: Normal / test mode, Semi-/fully automatic, Pushbutton / switch mode, Manual ON / ON-OFF; Twilight setting: 10 – 1000 lx; Time setting: 30 sec – 30 min; Basic light level function: No; Main light adjustable: No; Twilight setting TEACH: Yes; Constant-lighting control: No; Interconnection: Yes; Type of interconnection: Master/master, Master/slave; Interconnection via: Cable

**Manufacturer** Steinel

**Prod. No.** 079512

**Ordering designation** HF 360 COM1 - in-ceiling installation

Deliver, install and set ready for operation