**STEINEL Professional Presence detector**

**HF 360**

**DALI-2 APC - in-ceiling installation**

Dimensions (L x W x H): 112 x 120 x 120 mm; Manufacturer's Warranty: 5 years; Settings via: Remote control, DIP switches, Potentiometers, Smart Remote; With remote control: No; Version: DALI-2 APC - in-ceiling installation; PU1, EAN: 4007841079529; Type: Presence detector; Application, place: Indoors; Application, room: function room / ancillary room, kitchenette, stairwell, WC / washroom, Indoors; Colour: white; Colour, RAL: 9010; Includes corner wall mount: No; Installation site: ceiling; Installation: In-ceiling installation, Ceiling; IP-rating: IP20; Ambient temperature: from -25 up to 55 °C; Material: Plastic; Mains power supply: 230 V / 50 – 60 Hz; Steuerausgang, Dali: Broadcast 2x12 electronic ballasts; With bus coupling: Yes; Technology, sensors: High frequency, Light sensor; Mounting height: 2,50 – 3,50 m; Mounting height max.: 3,50 m; Optimum mounting height: 2,8 m; HF-system: 5,8 GHz; Detection: also through glass, wood and stud walls; Detection angle: 360 °; Angle of aperture: 140 °; Sneak-by guard: Yes; Capability of masking out individual segments: Yes; Electronic scalability: Yes; Mechanical scalability: No; Reach, radial: Ø 12 m (113 m²); Reach, tangential: Ø 12 m (113 m²); Transmitter power: < 1 mW; Functions: Normal / test mode, Semi-/fully automatic, Pushbutton / switch mode, Manual ON / ON-OFF, Constant-lighting control ON-OFF; Twilight setting: 10 – 1000 lx; Time setting: 30 sec – 30 min; Basic light level function: Yes; Basic light level function time: 1-60 min, all night; Main light adjustable: 50 - 100 %; Twilight setting TEACH: Yes; Constant-lighting control: Yes; Interconnection: Yes; Type of interconnection: Master/slave; Interconnection via: Cable; Product category: Presence detector

**Manufacturer** Steinel

**Prod. No.** 079529

**Ordering designation** HF 360 DALI-2 APC - in-ceiling installation

Deliver, install and set ready for operation