**STEINEL Professional Presence detector**

**IR Quattro 8m**

**KNX - in-ceiling installation V3**

Dimensions (L x W x H): 113 x 120 x 120 mm; With motion detector: Yes; Manufacturer's Warranty: 5 years; Settings via: ETS software, Remote control, Bus, Smart Remote; Version: KNX - in-ceiling installation; PU1, EAN: 4007841079390; Type: Presence detector; Application, place: Indoors; Application, room: one-person office, conference room / meeting room, duty room, recreation room, changing room, function room / ancillary room, kitchenette, Indoors; Colour: white; Colour, RAL: 9010; Includes corner wall mount: No; Installation site: ceiling; Installation: In-ceiling installation, Ceiling; IP-rating: IP20; Ambient temperature: 0 – 40 °C; Material: Plastic; With bus coupling: Yes; Technology, sensors: Photo-cell controller, passive infrared; Mounting height: 2,50 – 8,00 m; Mounting height max.: 8,00 m; Optimum mounting height: 2,8 m; Detection angle: 360 °; Angle of aperture: 100 °; Sneak-by guard: Yes; Capability of masking out individual segments: No; Electronic scalability: No; Mechanical scalability: Yes; Reach, radial: 5 x 5 m (25 m²); Reach, tangential: 7 x 7 m (49 m²); Reach, presence: 4 x 4 m (16 m²); Switching zones: 1760 switching zones; Twilight setting: 10 – 1000 lx; Time setting: 0 sec – 1092 min; Basic light level function: Yes; Main light adjustable: 0 - 100 %; Twilight setting TEACH: Yes; Constant-lighting control: Yes; KNX functions: Photo-cell controller, Basic light level function, Light level, HVAC output, Constant-lighting control, Light output 4x, Presence output, Day / night function, Logic gate; Interconnection: Yes; Type of interconnection: Master/master, Master/slave; Interconnection via: KNX bus; Rated current: 10 mA

**Manufacturer** Steinel

**Prod. No.** 079390

**Ordering designation** IR Quattro 8m KNX - in-ceiling installation

Deliver, install and set ready for operation