STEINEL Professional Sensor-switched LED outdoor light

DL Vario Quattro PRO S
warm white white

Dimensions (Ø x H): 310 x 69 mm;With lamp: Yes, STEINEL LED system;Manufacturer's Warranty: 5 years;Settings via: Potentiometers;With remote control: No;Version: warm white white;PU1, EAN: 4007841068202;Application, place: Outdoors;Application, room: corridor / aisle, function room / ancillary room, stairwell, outdoors, front door, courtyard & driveway, Indoors;Colour: white;Installation site: ceiling;Impact resistance: IK07;IP-rating: IP54;Protection class: II;Ambient temperature: from -20 up to 35 °C;Housing material: Plastic;Cover material: Plastic, structured;Mains power supply: 220 – 240 V / 50 – 60 Hz;Output: 14 W;Switching output 1, resistive: 500 W;Fluorescent lamps, electronic ballast: 500 W;Fluorescent lamps, uncorrected: 500 VA;Fluorescent lamps, series-corrected: 500 VA;Fluorescent lamps, parallel-corrected: 500 VA;Switching output 1, low-voltage halogen lamps: 500 VA;LED lamps < 2 W: 16 W;LED lamps > 2 W < 8 W: 64 W;LED lamps > 8 W: 64 W;Capacitive load in μF: 88 µF;Power consumption: 0,5 W;Mounting height max.: 6,00 m;Sneak-by guard: Yes;Capability of masking out individual segments: No;Electronic scalability: No;Mechanical scalability: Yes;Reach, detail: Reach adjustable from 2 - 8 m in 4 directions (90° in each);Reach, radial: 4 x 4 m (16 m²);Reach, tangential: 16 x 16 m (256 m²);Photo-cell controller: Yes;Luminous flux total product: 1430 lm;Measured luminos flux (360°): 1430 lm;Total product efficiency: 102 lm/W;Colour temperature: 3000 K;Colour variation LED: SDCM3;Lamp: LED cannot be replaced;LED life expectancy (max. °C): 50000 h;Service life LED L70B50 (25°): > 60000 h;Base: without;LED cooling system: Passive Thermo Control;Soft light start: Yes;Continuous light: selectable, 4h;Twilight setting: 2 – 1000 lx;Time setting: 5 sec – 30 min;Basic light level function: Yes;Basic light level function time: 10/30 min, all night;Twilight setting TEACH: No;Interconnection: Yes;Basic light level function in per cent: 10 %;Basic light level function percentage, from: 10 %;Interconnection via: Cable;Colour Rendering Index CRI: = 82;Optimum mounting height: 2,8 m;Detection angle: 360 °;Product category: Sensor-switched LED outdoor light

Manufacturer Steinel
Prod. No. 068202
Ordering designation DL Vario Quattro PRO S warm white white

Deliver, install and set ready for operation
