**STEINEL Professional Luminaire extérieur à détection**

**DL Vario Quattro PRO S**

**bl. chaud blanc**

Dimensions (Ø x H): 310 x 69 mm; With lamp: Oui, système d'éclairage LED STEINEL; Manufacturer's Warranty: 5 ans; Settings via: Potentiomètres; With remote control: Non; Version: bl. chaud blanc; PU1, EAN: 4007841068202; Application, place: Extérieur; Application, room: couloir / allée, espace fonctionnel / local annexe, cage d'escalier, extérieur, entrée, Cour et allée, Intérieur; Colour: blanc; Installation site: plafond; Impact resistance: IK07; IP-rating: IP54; Protection class: II; Ambient temperature: de -20 jusqu'à 35 °C; Housing material: Matière plastique; Cover material: Matière plastique structurée; Mains power supply: 220 – 240 V / 50 – 60 Hz; Output: 14 W; Switching output 1, resistive: 500 W; Fluorescent lamps, electronic ballast: 500 W; Fluorescent lamps, uncorrected: 500 VA; Fluorescent lamps, series-corrected: 500 VA; Fluorescent lamps, parallel-corrected: 500 VA; Switching output 1, low-voltage halogen lamps: 500 VA; LED lamps < 2 W: 16 W; LED lamps > 2 W < 8 W: 64 W; LED lamps > 8 W: 64 W; Capacitive load in μF: 88 µF; Power consumption: 0,5 W; Mounting height max.: 6,00 m; Sneak-by guard: Oui; Capability of masking out individual segments: Non; Electronic scalability: Non; Mechanical scalability: Oui; Reach, detail: Portée de 2 à 8 m réglable dans 4 directions (respectivement 90°); Reach, radial: 4 x 4 m (16 m²); Reach, tangential: 16 x 16 m (256 m²); Photo-cell controller: Oui; Luminous flux total product: 1430 lm; Measured luminos flux (360°): 1430 lm; Total product efficiency: 102 lm/W; Colour temperature: 3000 K; Colour variation LED: SDCM3; Lamp: LED non interchangeable; LED life expectancy (max. °C): 50000 h; Service life LED L70B50 (25°): > 60000; Base: sans; LED cooling system: Contrôle thermique passif; Soft light start: Oui; Continuous light: commutable, 4 h; Twilight setting: 2 – 1000 lx; Time setting: 5 s – 30 min; Basic light level function: Oui; Basic light level function time: 10/30 min, toute la nuit; Twilight setting TEACH: Non; Interconnection: Oui; Basic light level function in per cent: 10 %; Basic light level function percentage, from: 10 %; Interconnection via: Câble; Colour Rendering Index CRI: = 82; Optimum mounting height: 2,8 m; Detection angle: 360 °; Product category: Luminaire extérieur à détection

**Fabricant** Steinel

**Réf.** 068202

**Désignation commande** DL Vario Quattro PRO S bl. chaud blanc

Livrer, monter et régler pour être opérationnel