**STEINEL Professional LED outdoor light without sensor**

**GL 85 C 900**

**without motion detector**

Dimensions (L x W x H): 136 x 146 x 900 mm; With lamp: Yes, STEINEL LED system; Manufacturer's Warranty: 5 years; Settings via: App, Smartphone, Connect Bluetooth Mesh; With remote control: No; Version: without motion detector; PU1, EAN: 4007841078676; Application, place: Outdoors; Application, room: outdoors, garden; includes sheet of self-adhesive numbers: No; Installation site: Stand mounted; Impact resistance: IK03; IP-rating: IP44; Protection class: I; Ambient temperature: from -20 up to 40 °C; Housing material: Aluminium; Cover material: Plastic, opal; Mains power supply: 220 – 240 V / 50 – 60 Hz; Output: 9 W; Photo-cell controller: Yes; Luminous flux total product: 719 lm; Measured luminos flux (360°): 719 lm; Total product efficiency: 79,9 lm/W; Colour temperature: 3000 K; Colour variation LED: SDCM3; Lamp: LED cannot be replaced; Service life LED L70B50 (25°): > 60000 h; Drop in luminous flux in accordance with LM80: L70B50; Base: without; Soft light start: Yes; Functions: Motions sensor, Neighbouring group function; Main light adjustable: 0 - 100 %; Twilight setting TEACH: Yes; Interconnection: Yes; Type of interconnection: Master/slave; Interconnection via: Bluetooth Mesh Connect; Colour Rendering Index CRI: = 82; Product category: LED outdoor light without sensor

**Manufacturer** Steinel

**Prod. No.** 078676

**Ordering designation** GL 85 C 900 without motion detector

Deliver, install and set ready for operation