**STEINEL Professional Sensor-switched LED outdoor light**

**L 331 S**

**Anthracite**

Dimensions (L x W x H): 124 x 253 x 270 mm; With lamp: Yes, STEINEL LED system; Manufacturer's Warranty: 5 years; Settings via: Potentiometers; With remote control: No; Version: Anthracite; PU1, EAN: 4007841053093; Application, place: Outdoors; Application, room: outdoors, front door, all round the building, courtyard & driveway; Colour: Anthracite; Installation site: wall; Impact resistance: IK10; IP-rating: IP44; Protection class: II; Ambient temperature: -20 – 35 °C; Housing material: Plastic; Cover material: Plastic, opal; Mains power supply: 220 – 240 V / 50 – 60 Hz; Output: 8,4 W; Average rated life expectancy of power supply unit at 25°C: > 60000 h; Mounting height max.: 2,50 m; Slave modeselectable: No; Sneak-by guard: Yes; Capability of masking out individual segments: Yes; Electronic scalability: No; Mechanical scalability: No; Reach, radial: r = 2 m (13 m²); Reach, tangential: r = 7 m (154 m²); Photo-cell controller: Yes; Cover material: shrouds; Luminous flux total product: 711 lm; Measured luminos flux (360°): 711 lm; Total product efficiency: 85 lm/W; Colour temperature: 3000 K; Colour variation LED: SDCM3; Lamp: LED cannot be replaced; LED life expectancy (max. °C): 50000 h; Service life LED L70B50 (25°): > 60000 h; Base: without; LED cooling system: Passive Thermo Control; Soft light start: Yes; Continuous light: selectable, 4h; Functions: 4 programme settings geared to practical needs, can be selected on removable sensor module; Twilight setting: 2 – 1000 lx; Time setting: 5 sec – 15 min; Basic light level function: Yes; Basic light level function time: 10/30 min, all night; Interconnection: Yes; Type of interconnection: Master/master; Basic light level function in per cent: 10 %; Basic light level function percentage, from: 10 %; Basic light level function percentage, up to: 10 %; Interconnection via: Cable; Colour Rendering Index CRI: = 82; Optimum mounting height: 2 m; Detection angle: 360 °

**Manufacturer** Steinel

**Prod. No.** 053093

**Ordering designation** L 331 S Anthracite

Deliver, install and set ready for operation