STEINEL Professional Sensor-switched LED outdoor light

L 331 S
Anthracite

Dimensions (L x W x H): 124 x 253 x 270 mm;With lamp: Yes, STEINEL LED system;Manufacturer's Warranty: 5 years;Settings via: Potentiometers;With remote control: No;Version: Anthracite;PU1, EAN: 4007841053093;Application, place: Outdoors;Application, room: outdoors, front door, all round the building, courtyard & driveway;Colour: Anthracite;Package content: 1;Installation site: wall;Impact resistance: IK10;IP-rating: IP44;Protection class: II;Ambient temperature: from -20 up to 35 °C;Housing material: Plastic;Cover material: Plastic, opal;Mains power supply: 220 – 240 V / 50 – 60 Hz;Output: 8,4 W;Average rated life expectancy of power supply unit at 25°C: > 60000 h;Mounting height max.: 2,50 m;Slave modeselectable: No;Sneak-by guard: Yes;Capability of masking out individual segments: Yes;Electronic scalability: No;Mechanical scalability: No;Reach, radial: r = 2 m (13 m²);Reach, tangential: r = 7 m (154 m²);Photo-cell controller: Yes;Cover material: shrouds;Luminous flux total product: 711 lm;Measured luminos flux (360°): 711 lm;Total product efficiency: 85 lm/W;Colour temperature: 3000 K;Colour variation LED: SDCM3;Lamp: LED cannot be replaced;LED life expectancy (max. °C): 50000 h;Service life LED L70B50 (25°): > 60000 h;Base: without;LED cooling system: Passive Thermo Control;Soft light start: Yes;Continuous light: selectable, 4h;Functions: 4 programme settings geared to practical needs, can be selected on removable sensor module;Twilight setting: 2 – 1000 lx;Time setting: 5 sec – 15 min;Basic light level function: Yes;Basic light level function time: 10/30 min, all night;Interconnection: Yes;Type of interconnection: Master/master;Basic light level function in per cent: 10 %;Basic light level function percentage, from: 10 %;Basic light level function percentage, up to: 10 %;Interconnection via: Cable;Colour Rendering Index CRI: = 82;Optimum mounting height: 2 m;Detection angle: 360 °;Product category: Sensor-switched LED outdoor light

Manufacturer Steinel
Prod. No. 053093
Ordering designation L 331 S Anthracite

Deliver, install and set ready for operation
