**STEINEL Professional Lampada da esterno LED con sensore**

**L 691 S**

**PMMA antracite V2**

Dimensions (L x W x H): 126 x 291 x 303 mm; With lamp: Sì, sistema LED STEINEL; Manufacturer's Warranty: 5 anni; Settings via: Potenziometri; With remote control: No; Version: PMMA antracite; PU1, EAN: 4007841053031; Application, place: Esterno; Application, room: Esterno, ingressi di abitazioni, perimetro della casa, Cortili e passi carrai; Colour: antracite; Installation site: Parete; Impact resistance: IK07; IP-rating: IP44; Protection class: II; Ambient temperature: da -20 fino a 50 °C; Housing material: Alluminio; Cover material: Plastica opalina; Mains power supply: 220 – 240 V / 50 – 60 Hz; Output: 8,5 W; Average rated life expectancy of power supply unit at 25°C: > 60000; Mounting height max.: 2,50 m; Slave modeselectable: No; Sneak-by guard: Sì; Capability of masking out individual segments: Sì; Electronic scalability: No; Mechanical scalability: No; Reach, radial: r = 1.5 m (7 m²); Reach, tangential: r = 7 m (154 m²); Photo-cell controller: Sì; Cover material: calotte di copertura; Luminous flux total product: 576 lm; Measured luminos flux (360°): 576 lm; Total product efficiency: 68 lm/W; Colour temperature: 3000 K; Colour variation LED: SDCM3; Lamp: LED non sostituibile; Service life LED L70B50 (25°): > 60000; Base: senza; LED cooling system: Passive Thermo Control; Soft light start: Sì; Continuous light: commutabile, 4 ore; Functions: 4 impostazioni di programma sul modulo sensore amovibile, studiate in base alle esigenze pratiche; Twilight setting: 2 – 1000 lx; Time setting: 5 sec – 15 min; Basic light level function: Sì; Basic light level function time: 10/30 min, tutta la notte; Interconnection: Sì; Basic light level function in per cent: 10 %; Basic light level function percentage, from: 10 %; Basic light level function percentage, up to: 10 %; Interconnection via: Cavo; Colour Rendering Index CRI: = 82; Optimum mounting height: 2 m; Detection angle: 360 °; Product category: Lampada da esterno LED con sensore

**Produttore** Steinel

**Art. n.** 053031

**Denominazione ordine** L 691 S PMMA antracite

Consegnare, montare e impostare in modo che sia pronto alla messa in funzione