**STEINEL Professional LED indoor light without sensor**

**RS PRO 5100 C**

**without motion detector**

Dimensions (L x W x H): 1370 x 87 x 58 mm; With motion detector: No; Manufacturer's Warranty: 5 years; Version: without motion detector; PU1, EAN: 4007841079178; Colour: grey; Installation site: wall, ceiling; Installation: Wall, Ceiling, Surface wiring; Impact resistance: IK07; IP-rating: IP65; Protection class: II; Ambient temperature: from -20 up to 40 °C; Housing material: Plastic; Cover material: Plastic, structured; Mains power supply: 220 – 240 V / 50 – 60 Hz; Power consumption: 0,45 W; Electronic scalability: Yes; Luminous flux total product: 4250 lm; Total product efficiency: 137 lm/W; Colour temperature: 4000 K; Lamp: LED cannot be replaced; LED cooling system: Passive Thermo Control; Basic light level function: Yes; Basic light level function time: 1-60 min; Main light adjustable: 0 - 100 %; Interconnection via: Bluetooth Mesh; Lifetime LED according to IEC-62717 (L70): 100.000 h; Lifetime LED according to IEC-62717 (L80): 68.000 h; Lebensdauer LED nach IES TM-21 (L70): >60.000 h; Lifetime LED according to IES TM-21 (L80): >60.000 h; Fuse protection B10: 41; Fuse protection B16: 65; Fuse protection C10: 67; Fuse protection C16: 108; Output: 31 W; Colour Rendering Index CRI: = 82; Photobiological safety in accordance with EN 62471: RG1; Starting current, maximum: 14,8 A; Product category: LED indoor light without sensor

**Manufacturer** Steinel

**Prod. No.** 079178

**Ordering designation** RS PRO 5100 C without motion detector

Deliver, install and set ready for operation