**STEINEL Professional Indoor light without sensor**

**RS PRO 5150 C**

**without motion detector**

Dimensions (L x W x H): 1500 x 87 x 58 mm; With motion detector: No; Manufacturer's Warranty: 5 years; Version: without motion detector; PU1, EAN: 4007841058722; Colour: grey; Installation site: wall, ceiling; Installation: Ceiling; Impact resistance: IK07; IP-rating: IP65; Protection class: II; Ambient temperature: from -20 up to 40 °C; Housing material: Plastic; Cover material: Plastic, structured; Mains power supply: 220 – 240 V / 50 – 60 Hz; Power consumption: 0,45 W; Luminous flux total product: 5940 lm; Colour temperature: 4000 K; Lamp: LED cannot be replaced; Functions: Encrypted communication, Neighbouring group function, Free selection of the light value in a luminaire group, Adjustable fade time when switching on and off, Connection to central battery systems; Twilight setting: 2 – 2000 lx; Time setting: 5 sec – 60 min; Basic light level function: Yes; Basic light level function time: 1-60 min; Main light adjustable: 0 - 100 %; Interconnection: Yes; Interconnection via: Bluetooth Mesh; Lifetime LED according to IEC-62717 (L70): 100.000 h; Lifetime LED according to IEC-62717 (L80): 68.000 h; Lebensdauer LED nach IES TM-21 (L70): > 60.000 h; Lifetime LED according to IES TM-21 (L80): > 60.000 h; Fuse protection B10: 41; Fuse protection B16: 65; Fuse protection C10: 67; Fuse protection C16: 108; Basic light level function in per cent: 0 – 100 %; Output: 42 W; Photobiological safety in accordance with EN 62471: RG1; Starting current, maximum: 14,8 A; Product category: Indoor light without sensor

**Manufacturer** Steinel

**Prod. No.** 058722

**Ordering designation** RS PRO 5150 C without motion detector

Deliver, install and set ready for operation