**STEINEL Professional Sensor-switched LED indoor light**

**RS PRO 5150 SC 5C**

**5 Core (5-core through-wiring)**

Dimensions (L x W x H): 1500 x 87 x 58 mm; With motion detector: Yes; Manufacturer's Warranty: 5 years; Version: 5 Core (5-core through-wiring); PU1, EAN: 4007841079338; Colour: grey; Installation site: wall, ceiling; Installation: Ceiling; Impact resistance: IK07; IP-rating: IP65; Protection class: II; Ambient temperature: from -20 up to 40 °C; Housing material: Plastic; Cover material: Plastic, structured; Mains power supply: 220 – 240 V / 50 – 60 Hz; Power consumption: 0,45 W; Mounting height max.: 3,50 m; Electronic scalability: Yes; Luminous flux total product: 5940 lm; Colour temperature: 4000 K; Lamp: LED cannot be replaced; Functions: Encrypted communication, Neighbouring group function, Free selection of the light value in a luminaire group, Adjustable fade time when switching on and off, Connection to central battery systems, Motions sensor, Light sensor, Orientation light; Twilight setting: 2 – 2000 lx; Time setting: 5 sec – 60 min; Basic light level function: Yes; Basic light level function time: 1-60 min; Main light adjustable: 0 - 100 %; Interconnection: Yes; Interconnection via: Bluetooth Mesh; Lifetime LED according to IEC-62717 (L70): 100.000 h; Lifetime LED according to IEC-62717 (L80): 68.000 h; Lebensdauer LED nach IES TM-21 (L70): > 60.000 h; Lifetime LED according to IES TM-21 (L80): > 60.000 h; Fuse protection B10: 41; Fuse protection B16: 65; Fuse protection C10: 67; Fuse protection C16: 108; Basic light level function in per cent: 0 – 100 %; Output: 42 W; Photobiological safety in accordance with EN 62471: RG1; Starting current, maximum: 14,8 A; Angle of aperture: 160 °; Detection angle: 360 °; Product category: Sensor-switched LED indoor light

**Manufacturer** Steinel

**Prod. No.** 079338

**Ordering designation** RS PRO 5150 SC 5C 5 Core (5-core through-wiring)

Deliver, install and set ready for operation