**STEINEL Professional Lampada a sensore per interno LED**

**RS PRO R20 basic Q SC**

**Bianco neutro**

Dimensions (L x W x H): 300 x 300 x 52 mm; With lamp: Sì, sistema LED STEINEL; With motion detector: Sì; Manufacturer's Warranty: 5 anni; Settings via: Bluetooth; With remote control: No; Version: Bianco neutro; PU1, EAN: 4007841067830; Application, place: Interni; Application, room: corridoio / pianerottolo, spogliatoi, locale multiuso / di servizio, cucinette, vano scala, Interni; Colour: bianco; includes sheet of self-adhesive numbers: No; Installation site: Parete, soffitto; Installation: Parete, Soffitto, In superficie; Impact resistance: IK07; IP-rating: IP40; Protection class: II; Ambient temperature: da -20 fino a 40 °C; Housing material: Plastica; Cover material: PC opalina; Mains power supply: 220 – 240 V / 50 – 60 Hz; Power consumption: 0,3 W; Mounting height max.: 4,00 m; HF-system: 5,8 GHz; Slave modeselectable: Sì; Detection: anche attraverso vetro, legno e pareti in materiale leggero; Capability of masking out individual segments: Sì; Electronic scalability: Sì; Mechanical scalability: No; Reach, radial: Ø 10 m (79 m²); Reach, tangential: Ø 10 m (79 m²); Photo-cell controller: Sì; Transmitter power: < 1 mW; Luminous flux total product: 1970 lm; Total product efficiency: 129 lm/W; Colour temperature: 4000 K; Colour variation LED: SDCM3; Lamp: LED non sostituibile; Base: senza; LED cooling system: Passive Thermo Control; Soft light start: Sì; Continuous light: commutabile; Functions: Parametrizzazione di gruppi, Manuale ON / ON-OFF, Funzione di gruppo vicino, Luce di orientamento, Sensore di movimento, Sensore di luce, Comunicazione criptata, Selezione libera del valore della luce in un gruppo di apparecchi, Tempo di dissolvenza regolabile quando si accende e si spegne, Sovracomando Master/Slave, Funzione presenza, Regolazione della luce constante ON-OFF; Twilight setting: 2 – 2000 lx; Time setting: 5 sec – 60 min; Basic light level function: Sì; Basic light level function, detail: Luce di effetto LED; Basic light level function time: 1-60 min; Main light adjustable: 0 - 100 %; Twilight setting TEACH: Sì; Interconnection: Sì; Type of interconnection: master/master; Interconnection via: Bluetooth Mesh; Lifetime LED according to IEC-62717 (L70): 100000; Lifetime LED according to IEC-62717 (L80): 73000; Durata dei LED secondo IES TM-21 (L70): 60000; Lifetime LED according to IES TM-21 (L80): 60000; Fuse protection B10: 46; Fuse protection B16: 74; Fuse protection C10: 77; Fuse protection C16: 122; Basic light level function in per cent: 0 – 100 %; Output: 15,3 W; Colour Rendering Index CRI: = 82; Photobiological safety in accordance with EN 62471: RG1; Starting current, maximum: 13 A; Angle of aperture: 160 °; IP-rating, ceiling: IP40; Detection angle: 360 °; Product category: Lampada a sensore per interno LED

**Produttore** Steinel

**Art. n.** 067830

**Denominazione ordine** RS PRO R20 basic Q SC Bianco neutro

Consegnare, montare e impostare in modo che sia pronto alla messa in funzione