STEINEL Professional Sensor-switched LED floodlight

XLED PRO 240 S
warm white black V2

Dimensions (L x W x H): 161 x 180 x 223 mm;With lamp: Yes, STEINEL LED system;With motion detector: Yes;Manufacturer's Warranty: 5 years;Settings via: Potentiometers;Version: warm white black;PU1, EAN: 4007841068110;Application, place: Outdoors;Application, room: outdoors, all round the building, terrace / balcony, courtyard & driveway;Includes corner wall mount: No;Installation site: wall, corner;Installation: Wall, corner, Surface wiring;Impact resistance: IK03;IP-rating: IP44;Protection class: II;Ambient temperature: from -20 up to 40 °C;Housing material: HCMC;Cover material: Plastic, opal;Mains power supply: 220 – 240 V / 50 – 60 Hz;Mounting height max.: 6,00 m;Sneak-by guard: Yes;Capability of masking out individual segments: Yes;Electronic scalability: No;Mechanical scalability: No;Reach, radial: r = 3 m (19 m²);Reach, tangential: r = 12 m (302 m²);Photo-cell controller: Yes;Cover material: shrouds;Luminous flux total product: 2124 lm;Measured luminos flux (360°): 2124 lm;Total product efficiency: 110 lm/W;Colour temperature: 3000 K;Colour variation LED: SDCM3;Lamp: LED cannot be replaced;Service life LED L70B50 (25°): > 60000 h;LED cooling system: HCMC (High Conductive Magnesium Composite);Soft light start: No;Continuous light: selectable;Twilight setting: 2 – 2000 lx;Time setting: 10 sec – 15 min;Basic light level function: No;Main light adjustable: No;Twilight setting TEACH: No;Interconnection: Yes;Interconnection via: Cable;Interconnection, number: maximum of 10 floodlights;Output: 19,3 W;Colour Rendering Index CRI: = 82;Optimum mounting height: 2 m;Detection angle: 240 °;Product category: Sensor-switched LED floodlight;Energy efficiency class of light source: E

Manufacturer Steinel
Prod. No. 068110
Ordering designation XLED PRO 240 S warm white black

Deliver, install and set ready for operation
