**STEINEL Professional Lampada a sensore per interno LED**

**RS PRO S30 SC**

**PMMA Bianco neutro**

Dimensions (Ø x H): 350 x 83 mm; With lamp: Sì, sistema LED STEINEL; With motion detector: Sì; Manufacturer's Warranty: 5 anni; Settings via: Bluetooth; With remote control: No; Version: PMMA Bianco neutro; PU1, EAN: 4007841068042; Application, place: Interni; Application, room: spogliatoi, cucinette, Interni, Esterno, WC / docce, vano scala, locale multiuso / di servizio, corridoio / pianerottolo; Colour: argento; includes sheet of self-adhesive numbers: No; Installation site: Parete, soffitto; Installation: Parete, Soffitto, In superficie; Impact resistance: IK07; IP-rating: IP20; Protection class: II; Ambient temperature: da -20 fino a 40 °C; Housing material: Alluminio; Cover material: Plastica opalina; Mains power supply: 220 – 240 V / 50 – 60 Hz; Power consumption: 0,39 W; Mounting height max.: 4,00 m; HF-system: 5,8 GHz; Slave modeselectable: Sì; Detection: anche attraverso vetro, legno e pareti in materiale leggero; Capability of masking out individual segments: Sì; Electronic scalability: Sì; Mechanical scalability: No; Reach, radial: Ø 10 m (79 m²); Reach, tangential: Ø 10 m (79 m²); Photo-cell controller: Sì; Transmitter power: < 1 mW; Luminous flux total product: 2747 lm; Total product efficiency: 106 lm/W; Colour temperature: 4000 K; Colour variation LED: SDCM3; Lamp: LED non sostituibile; Base: altro; LED cooling system: Passive Thermo Control; Soft light start: Sì; Continuous light: commutabile, 4 ore; Functions: Funzione di gruppo vicino, Funzione presenza, Parametrizzazione di gruppi, Manuale ON / ON-OFF, Connessione a sistemi di batterie centrali, Sensore di movimento, Funzione DIM, Tempo di dissolvenza regolabile quando si accende e si spegne, Selezione libera del valore della luce in un gruppo di apparecchi, Modalità normale / modalità test, Luce di orientamento, Logica del rilevatore di presenza, Comunicazione criptata, Regolazione della luce constante ON-OFF, Sovracomando Master/Slave, Monitoraggio dei dati; Twilight setting: 2 – 2000 lx; Time setting: 5 sec – 30 min; Basic light level function: Sì; Basic light level function, detail: Luce di effetto LED; Basic light level function time: 10-30 min, tutto il giorno, Tutta la notte; Main light adjustable: 5 - 100 %; Twilight setting TEACH: Sì; Interconnection: Sì; Type of interconnection: master/master; Interconnection via: Bluetooth Mesh; Lifetime LED according to IEC-62717 (L70): 100.000 h; Lifetime LED according to IEC-62717 (L80): 74.000 h; Durata dei LED secondo IES TM-21 (L70): >60.000 h; Lifetime LED according to IES TM-21 (L80): >60.000 h; Fuse protection B10: 36; Fuse protection B16: 58; Fuse protection C10: 61; Fuse protection C16: 97; Basic light level function in per cent: 10 – 50 %; Output: 25,8 W; Starting current, maximum: 16,5 A; Angle of aperture: 160 °; Detection angle: 360 °; Product category: Lampada a sensore per interno LED

**Produttore** Steinel

**Art. n.** 068042

**Denominazione ordine** RS PRO S30 SC PMMA Bianco neutro

Consegnare, montare e impostare in modo che sia pronto alla messa in funzione