**STEINEL Professional Sensor-switched LED indoor light**

**RS PRO S30 SC - Multipack (5 ea.)**

**PMMA Neutral white**

Dimensions (Ø x H): 350 x 83 mm; With lamp: Yes, STEINEL LED system; With motion detector: Yes; Manufacturer's Warranty: 5 years; Settings via: Bluetooth, App; With remote control: No; Version: PMMA Neutral white; PU1, EAN: 4007841079710; Application, place: Indoors; Application, room: changing room, kitchenette, Indoors, outdoors, WC / washroom, stairwell, function room / ancillary room, corridor / aisle; Colour: Silver; includes sheet of self-adhesive numbers: No; Installation site: ceiling, wall; Installation: Wall, Ceiling; Impact resistance: IK07; IP-rating: IP20; Protection class: II; Ambient temperature: from -20 up to 40 °C; Housing material: Aluminium; Cover material: Plastic, opal; Mains power supply: 220 – 240 V / 50 – 60 Hz; Power consumption: 0,39 W; Mounting height max.: 4,00 m; HF-system: 5,8 GHz; Slave modeselectable: Yes; Detection: also through glass, wood and stud walls; Capability of masking out individual segments: Yes; Electronic scalability: Yes; Mechanical scalability: No; Reach, radial: Ø 10 m (79 m²); Reach, tangential: Ø 10 m (79 m²); Photo-cell controller: Yes; Transmitter power: < 1 mW; Luminous flux total product: 2747 lm; Total product efficiency: 106 lm/W; Colour temperature: 4000 K; Colour variation LED: SDCM3; Lamp: LED cannot be replaced; Base: without; LED cooling system: Passive Thermo Control; Soft light start: Yes; Continuous light: selectable, 4h; Functions: Neighbouring group function, Presence function, Group parameterisation, Manual ON / ON-OFF, Connection to central battery systems, Motions sensor, DIM function, Adjustable fade time when switching on and off, Free selection of the light value in a luminaire group, Normal / test mode, Orientation light, Presence detector logic, Encrypted communication, Constant-lighting control ON-OFF, Master/slave override, Data monitoring; Twilight setting: 2 – 2000 lx; Time setting: 5 sec – 60 min; Basic light level function: Yes; Basic light level function, detail: LED effect light; Basic light level function time: 1-60 min; Main light adjustable: 5 - 100 %; Twilight setting TEACH: Yes; Interconnection: Yes; Type of interconnection: Master/master; Interconnection via: Bluetooth Mesh Connect; Lifetime LED according to IEC-62717 (L70): 100.000 h; Lifetime LED according to IEC-62717 (L80): 74.000 h; Lebensdauer LED nach IES TM-21 (L70): >60.000 h; Lifetime LED according to IES TM-21 (L80): >60.000 h; Fuse protection B10: 36; Fuse protection B16: 58; Fuse protection C10: 61; Fuse protection C16: 97; Basic light level function in per cent: 7 – 100 %; Output: 25,8 W; Starting current, maximum: 16,5 A; Angle of aperture: 160 °; Detection angle: 360 °; Product category: Sensor-switched LED indoor light

**Manufacturer** Steinel

**Prod. No.** 079710

**Ordering designation** RS PRO S30 SC - Multipack (5 ea.) PMMA Neutral white

Deliver, install and set ready for operation