**STEINEL Professional Sensor-switched LED indoor light**

**RS PRO S30 Q SC**

**warm white**

Dimensions (L x W x H): 331 x 331 x 56 mm; With lamp: Yes, STEINEL LED system; With motion detector: Yes; Manufacturer's Warranty: 5 years; Settings via: Bluetooth; With remote control: No; Version: warm white; PU1, EAN: 4007841067526; Application, place: Indoors; Application, room: corridor / aisle, changing room, function room / ancillary room, kitchenette, stairwell, WC / washroom, outdoors, Indoors; Colour: Silver; includes sheet of self-adhesive numbers: No; Installation site: wall, ceiling; Installation: Wall, Ceiling, Surface wiring; Impact resistance: IK03; IP-rating: IP20; Protection class: II; Ambient temperature: from -20 up to 40 °C; Housing material: Aluminium; Cover material: Plastic, opal; Mains power supply: 220 – 240 V / 50 – 60 Hz; Power consumption: 0,39 W; Mounting height max.: 4,00 m; Slave modeselectable: Yes; Detection: also through glass, wood and stud walls; Capability of masking out individual segments: Yes; Electronic scalability: Yes; Mechanical scalability: No; Reach, radial: Ø 10 m (79 m²); Reach, tangential: Ø 10 m (79 m²); Photo-cell controller: Yes; Transmitter power: < 1 mW; Luminous flux total product: 2801 lm; Total product efficiency: 108 lm/W; Colour temperature: 3000 K; Colour variation LED: SDCM3; Lamp: LED cannot be replaced; Base: without; LED cooling system: Passive Thermo Control; Soft light start: Yes; Continuous light: selectable; Functions: Group parameterisation, Manual ON / ON-OFF, Neighbouring group function, Presence function, Motions sensor, Connection to central battery systems, DIM function, Adjustable fade time when switching on and off, Light sensor, Normal / test mode, Orientation light, Presence detector logic, Encrypted communication; Twilight setting: 2 – 2000 lx; Time setting: 5 sec – 60 min; Basic light level function: Yes; Basic light level function, detail: LED effect light; Basic light level function time: 1-60 min; Main light adjustable: Yes; Twilight setting TEACH: Yes; Interconnection: Yes; Type of interconnection: Master/master; Interconnection via: Bluetooth Mesh Connect; Lifetime LED according to IEC-62717 (L70): 100.000 h; Lifetime LED according to IEC-62717 (L80): 74.000 h; Lebensdauer LED nach IES TM-21 (L70): >60.000 h; Lifetime LED according to IES TM-21 (L80): >60.000 h; Fuse protection B10: 36; Fuse protection B16: 58; Fuse protection C10: 61; Fuse protection C16: 97; Basic light level function in per cent: 7 – 100 %; Output: 26 W; Colour Rendering Index CRI: = 82; Starting current, maximum: 16,5 A; Angle of aperture: 160 °; Detection angle: 360 °; Product category: Sensor-switched LED indoor light

**Manufacturer** Steinel

**Prod. No.** 067526

**Ordering designation** RS PRO S30 Q SC warm white

Deliver, install and set ready for operation