**STEINEL Professional Multisensor**

**Multisensor Air**

**BT IPD - concealed**

Dimensions (L x W x H): 51 x 123 x 123 mm; With motion detector: No; Manufacturer's Warranty: 5 years; Settings via: Smartphone, Tablet, Connect Bluetooth Mesh; With remote control: No; Version: BT IPD - concealed; PU1, EAN: 4007841084264; Type: Other; Application, place: Indoors; Application, room: open-plan office, hotel room, classroom, conference room / meeting room; Colour: white; Includes corner wall mount: No; Installation site: ceiling; Installation: Concealed wiring, Ceiling; IP-rating: IP20; Ambient temperature: 0 – 50 °C; Material: Plastic; Mains power supply: 50 – 60 Hz; Technology, sensors: CO2, Noise level, Air pressure, Air humidity, Light sensor, Temperature, VOC; Mounting height: 2 – 12 m; Mounting height max.: 12,00 m; Optimum mounting height: 2,8 m; Twilight setting: 2 – 2000 lx; Main light adjustable: Yes; Twilight setting TEACH: Yes; Constant-lighting control: No; Interconnection: Yes; Interconnection via: Bluetooth Mesh Connect

**Manufacturer** Steinel

**Prod. No.** 084264

**Ordering designation** Multisensor Air BT IPD - concealed

Deliver, install and set ready for operation