**STEINEL Professional Multisensor**

**Multisensor True Presence**

**BT IPD - concealed V2**

Dimensions (L x W x H): 51 x 142 x 142 mm; With motion detector: Yes; Manufacturer's Warranty: 5 years; Settings via: Smartphone, Tablet, Connect Bluetooth Mesh; With remote control: No; Version: BT IPD - concealed; PU1, EAN: 4007841084127; Type: Presence detector; Application, place: Indoors; Application, room: open-plan office, hotel room, classroom, conference room / meeting room; Colour: white; Includes corner wall mount: No; Installation site: ceiling; Installation: Concealed wiring; IP-rating: IP20; Ambient temperature: 0 – 50 °C; Material: Plastic; Mains power supply: 50 – 60 Hz; Power consumption: 1 W; Technology, sensors: Light sensor, High frequency, Air humidity, Air pressure, Temperature, VOC, Noise level, CO2; Mounting height: 2 – 12 m; Mounting height max.: 12,00 m; Optimum mounting height: 2,8 m; Montagehöhe max. True Presence Erfassung: 4,00 m; HF-system: 7,2 GHz; Detection: also through glass, wood and stud walls; Detection angle: 360 °; Angle of aperture: 160 °; Capability of masking out individual segments: No; Electronic scalability: Yes; Mechanical scalability: No; Reach, radial: Ø 15 m (177 m²); Reach, tangential: Ø 15 m (177 m²); Reach, presence: Ø 15 m (177 m²); True Presence reach: Ø 9 m (64 m²); Transmitter power: < 10 mW; Twilight setting: 2 – 2000 lx; Main light adjustable: Yes; Twilight setting TEACH: Yes; Constant-lighting control: No; Interconnection: Yes; Interconnection via: Bluetooth Mesh Connect

**Manufacturer** Steinel

**Prod. No.** 084127

**Ordering designation** Multisensor True Presence BT IPD - concealed

Deliver, install and set ready for operation