**STEINEL Professional Multisensor**

**Multisensor True Presence**

**IP - concealed V2**

Dimensions (L x W x H): 123 x 123 x 53 mm; With motion detector: Yes; Manufacturer's Warranty: 5 years; Settings via: Connect Bluetooth Mesh, Web-Interface; With remote control: No; Version: IP - concealed; PU1, EAN: 4007841081867; Type: Presence detector; Application, place: Indoors; Application, room: open-plan office, hotel room, classroom, conference room / meeting room; Colour: white; Includes corner wall mount: No; Installation site: ceiling; Installation: Concealed wiring; IP-rating: IP20; Ambient temperature: 0 – 50 °C; Material: Plastic; Power consumption: 1 W; Power supply, detail: Passive PoE SELV, standard PoE (IEEE 802.3 af); With bus coupling: Yes; Technology, sensors: Light sensor, High frequency, Air humidity, Air pressure, Temperature, VOC, Noise level, CO2; Mounting height: 2 – 12 m; Mounting height max.: 12,00 m; Optimum mounting height: 2,8 m; Montagehöhe max. True Presence Erfassung: 4,00 m; HF-system: 7,2 GHz; Detection: also through glass, wood and stud walls; Detection angle: 360 °; Angle of aperture: 160 °; Capability of masking out individual segments: No; Electronic scalability: Yes; Mechanical scalability: No; Reach, radial: Ø 15 m (177 m²); Reach, tangential: Ø 15 m (177 m²); Reach, presence: Ø 15 m (177 m²); True Presence reach: Ø 9 m (64 m²); Transmitter power: < 10 mW; Functions: Motions sensor, Light sensor; Twilight setting: 2 – 2000 lx; Main light adjustable: Yes; Twilight setting TEACH: Yes; Interconnection: Yes; Interconnection via: Bluetooth Mesh Connect

**Manufacturer** Steinel

**Prod. No.** 081867

**Ordering designation** Multisensor True Presence IP - concealed

Deliver, install and set ready for operation