**STEINEL Professional Presence detector**

**IR Quattro HD-2 24m**

**BT IPD - concealed**

Dimensions (L x W x H): 69 x 103 x 103 mm; Manufacturer's Warranty: 5 years; Settings via: Bluetooth; With remote control: No; Version: BT IPD - concealed; PU1, EAN: 4007841064396; Type: Presence detector; Application, place: Indoors; Application, room: lecture hall, classroom, open-plan office, high-bay warehouse, production facilities, conference room / meeting room, duty room, recreation room, changing room, reception / lobby, sports hall, multi-storey / underground car park, dining hall / staff restaurant, Indoors; Colour: white; Colour, RAL: 9003; Includes corner wall mount: No; Installation site: ceiling; Installation: Concealed wiring, Ceiling; IP-rating: IP20; Ambient temperature: -20 – 50 °C; Material: Plastic; Mains power supply: 220 – 240 V / 50 – 60 Hz; Power consumption: 0,3 W; Technology, sensors: Light sensor, passive infrared; Mounting height: 2,50 – 10,00 m; Mounting height max.: 10,00 m; Optimum mounting height: 2,8 m; Detection angle: 360 °; Angle of aperture: 160 °; Sneak-by guard: Yes; Capability of masking out individual segments: Yes; Electronic scalability: Yes; Mechanical scalability: Yes; Reach, radial: 9 x 9 m (81 m²); Reach, tangential: 24 x 24 m (576 m²); Reach, presence: 9 x 9 m (81 m²); Twilight setting: 2 – 2000 lx; Time setting: 5 sec – 60 min; Basic light level function: No; Main light adjustable: No; Twilight setting TEACH: No; Constant-lighting control: No; Interconnection: Yes; Interconnection via: Bluetooth Mesh Connect

**Manufacturer** Steinel

**Prod. No.** 064396

**Ordering designation** IR Quattro HD-2 24m BT IPD - concealed

Deliver, install and set ready for operation