**STEINEL Professional LED floodlight without sensor**

**XLED PRO ONE Max**

**without motion detector - white**

Dimensions (L x W x H): 202 x 259 x 226 mm; With lamp: Yes, STEINEL LED system; With motion detector: No; Manufacturer's Warranty: 5 years; Version: without motion detector - white; PU1, EAN: 4007841086824; Application, place: Outdoors; Application, room: outdoors, garden, front door, courtyard & driveway, all round the building; Colour: white; Includes corner wall mount: No; Installation site: ceiling, wall; Installation: Surface wiring, Wall; Impact resistance: IK03; IP-rating: IP44; Protection class: I; Ambient temperature: from -20 up to 40 °C; Housing material: Aluminium; Cover material: Glass transparent; Mains power supply: 220 – 240 V / 50 – 60 Hz; Photo-cell controller: No; Cover material: shrouds; Luminous flux total product: 6093 lm; Measured luminos flux (360°): 6093 lm; Total product efficiency: 123 lm/W; Colour temperature: 3000 K; Colour variation LED: SDCM3; Lamp: LED cannot be replaced; Service life LED L70B50 (25°): > 36000 h; LED cooling system: Passive Thermo Control; Functions: Relay output; Basic light level function: No; Main light adjustable: No; Twilight setting TEACH: No; Interconnection: Yes; Type of interconnection: Master/slave; Interconnection via: Cable; Output: 49,4 W; Colour Rendering Index CRI: = 80; Product category: LED floodlight without sensor; Energieeffizienzklasse Lichtquelle: E

**Manufacturer** Steinel

**Prod. No.** 086824

**Ordering designation** XLED PRO ONE Max without motion detector - white

Deliver, install and set ready for operation