STEINEL Professional Presence detector

LuxMaster IR Quattro HD-2 24m
DALI-2 APC - surface

Dimensions (L x W x H): 64 x 123 x 123 mm;Manufacturer's Warranty: 5 years;Settings via: Bluetooth;With remote control: No;Version: DALI-2 APC - surface;PU1, EAN: 4007841064365;Type: Presence detector;Application, place: Indoors;Application, room: lecture hall, classroom, open-plan office, high-bay warehouse, production facilities, conference room / meeting room, duty room, recreation room, changing room, reception / lobby, sports hall, multi-storey / underground car park, dining hall / staff restaurant, Indoors;Colour: white;Colour, RAL: 9003;Includes corner wall mount: No;Installation site: ceiling;Installation: Surface wiring, Ceiling;IP-rating: IP54;Ambient temperature: from -20 up to 50 °C;Material: Plastic;Mains power supply: 220 – 240 V / 50 – 60 Hz;Power consumption: 0,3 W;Power supply, detail: max. 64 users;Number of Dali users: 64;Control output, Dali: Addressable / broadcast 64 electronic ballasts;Technology, sensors: Mixed light metering, passive infrared;Voltage range (min): 220 V;Voltage range (max): 240 V;Mounting height: 2,50 – 10,00 m;Mounting height max.: 10,00 m;Optimum mounting height: 2,8 m;Detection angle: 360 °;Angle of aperture: 360 °;Sneak-by guard: Yes;Capability of masking out individual segments: Yes;Electronic scalability: Yes;Mechanical scalability: Yes;Reach, radial: 9 x 9 m (81 m²);Reach, tangential: 24 x 24 m (576 m²);Reach, presence: 9 x 9 m (81 m²);Switching zones: 5200 switching zones;Functions: Selecting programmed lighting scenarios, Semi-/fully automatic, Constant-lighting control ON-OFF, Lighting scenario, Manual ON / ON-OFF, Neighbouring group function, Normal / test mode, TouchDIM function;Twilight setting: 2 – 2000 lx;Time setting: 5 sec – 30 min;Basic light level function: Yes;Basic light level function time: 1-60 min, all night;Main light adjustable: 10 - 100 %;Twilight setting TEACH: Yes;Constant-lighting control: Yes;Interconnection: Yes;Interconnection via: Bluetooth, DALI bus;Product category: Presence detector

Manufacturer Steinel
Prod. No. 064365
Ordering designation LuxMaster IR Quattro HD-2 24m DALI-2 APC - surface

Deliver, install and set ready for operation
