STEINEL Professional Motion and Presence Detector

PD-24 ECO
COM1 - concealed  black

Dimensions (Ø x H): 109 x 74 mm;With motion detector: Yes;Manufacturer's Warranty: 5 years;Settings via: Remote control, Smart Remote, Potentiometers;With remote control: No;Version: COM1 - concealed  black;PU1, EAN: 4007841087869;Type: Motion and Presence Detector;Application, place: Indoors;Application, room: one-person office, function room / ancillary room, Indoors, warehouse;Colour: black;Includes corner wall mount: No;Installation site: ceiling;Installation: Concealed wiring, Ceiling;IP-rating: IP20;Ambient temperature: from -20 up to 50 °C;Material: Plastic;Switching output 1, resistive: 2000 W;Switching output 1, number of LEDs / fluorescent lamps: 50 pcs.;LED lamps > 8 W: 500 W;Capacitive load in μF: 176 µF;Technology, sensors: passive infrared, Mixed light metering;Mounting height: 2 – 10,00 m;Mounting height max.: 10,00 m;Optimum mounting height: 2,8 m;Detection angle: 360 °;Capability of masking out individual segments: Yes;Electronic scalability: No;Mechanical scalability: No;Reach, radial: Ø 5.5 m (24 m²);Reach, tangential: Ø 24 m (452 m²);Reach, presence: Ø 7.5 m (44 m²);Switching zones: 1436 switching zones;Cover material: shrouds;Functions: Motions sensor, Light sensor, Presence function, Presence detector logic, Semi-/fully automatic, Normal / test mode, Potentiometer, Relay output;Twilight setting: 2 – 1000 lx;Time setting: 5 sec – 60 min;Main light adjustable: No;Twilight setting TEACH: Yes;Constant-lighting control: No;Type of interconnection: Master/master;Interconnection via: Cable;Interconnection, number: max. 10 sensors;Product category: Motion and Presence Detector

Manufacturer Steinel
Prod. No. 087869
Ordering designation PD-24 ECO COM1 - concealed  black

Deliver, install and set ready for operation
