**STEINEL Professional Motion and Presence Detector**

**PD-24 ECO**

**KNX - in-ceiling installation, white**

With motion detector: Yes; Manufacturer's Warranty: 5 years; Settings via: Bus, ETS software, Smart Remote; With remote control: No; Version: KNX - in-ceiling installation, white; PU1, EAN: 4007841088033; Type: Motion and Presence Detector; Application, place: Indoors; Application, room: one-person office, function room / ancillary room, Indoors, warehouse; Colour: white; Includes corner wall mount: No; Installation site: ceiling; Installation: In-ceiling installation, Ceiling; IP-rating: IP20; Ambient temperature: -20 – 50 °C; Material: Plastic; With bus coupling: Yes; Technology, sensors: passive infrared, Light sensor; Mounting height: 2 – 4 m; Mounting height max.: 4,00 m; Optimum mounting height: 2,8 m; Detection angle: 360 °; Capability of masking out individual segments: Yes; Electronic scalability: No; Mechanical scalability: No; Reach, radial: Ø 5.5 m (24 m²); Reach, tangential: Ø 24 m (452 m²); Reach, presence: Ø 7.5 m (44 m²); Switching zones: 1436 switching zones; Abdeckmaterial Lieferumfang: shrouds; Functions: Motions sensor, Light sensor, Presence function, Presence detector logic; Twilight setting: 2 – 800 lx; KNX functions: Light level, Light output 2x, Constant-lighting control, Photo-cell controller, Basic light level function, HVAC output, Logic gate, Presence output, Sabotage protection, Day / night function; Type of interconnection: Master/master; Interconnection via: Cable; Rated current: 10 mA

**Manufacturer** Steinel

**Prod. No.** 088033

**Ordering designation** PD-24 ECO KNX - in-ceiling installation, white

Deliver, install and set ready for operation