**STEINEL Professional LED floodlight without sensor**

**XLED PRO 240**

**black V2**

Dimensions (L x W x H): 161 x 180 x 199 mm; With lamp: Yes, STEINEL LED system; With motion detector: No; Manufacturer's Warranty: 5 years; Version: black; PU1, EAN: 4007841068097; Application, place: Outdoors; Application, room: outdoors, all round the building, terrace / balcony, courtyard & driveway; Includes corner wall mount: No; Installation site: wall, corner; Installation: Wall, corner, Surface wiring; Impact resistance: IK03; IP-rating: IP44; Protection class: II; Ambient temperature: from -20 up to 40 °C; Housing material: HCMC; Cover material: Plastic, opal; Mains power supply: 220 – 240 V / 50 – 60 Hz; Luminous flux total product: 2124 lm; Measured luminos flux (360°): 2124 lm; Total product efficiency: 110 lm/W; Colour temperature: 3000 K; Colour variation LED: SDCM3; Lamp: LED cannot be replaced; Service life LED L70B50 (25°): > 60000 h; LED cooling system: HCMC (High Conductive Magnesium Composite); Soft light start: No; Basic light level function: No; Main light adjustable: No; Interconnection: No; Output: 19,3 W; Colour Rendering Index CRI: = 82; Product category: LED floodlight without sensor; Energieeffizienzklasse Lichtquelle: E

**Manufacturer** Steinel

**Prod. No.** 068097

**Ordering designation** XLED PRO 240 black

Deliver, install and set ready for operation