STEINEL Professional LED floodlight without sensor

XLED PRO 240
black V2

Dimensions (L x W x H): 161 x 180 x 199 mm;With lamp: Yes, STEINEL LED system;With motion detector: No;Manufacturer's Warranty: 5 years;Version: black;PU1, EAN: 4007841068097;Application, place: Outdoors;Application, room: outdoors, all round the building, terrace / balcony, courtyard & driveway;Includes corner wall mount: No;Installation site: wall, corner;Installation: Wall, corner, Surface wiring;Impact resistance: IK03;IP-rating: IP44;Protection class: II;Ambient temperature: from -20 up to 40 °C;Housing material: HCMC;Cover material: Plastic, opal;Mains power supply: 220 – 240 V / 50 – 60 Hz;Luminous flux total product: 2124 lm;Measured luminos flux (360°): 2124 lm;Total product efficiency: 110 lm/W;Colour temperature: 3000 K;Colour variation LED: SDCM3;Lamp: LED cannot be replaced;Service life LED L70B50 (25°): > 60000 h;LED cooling system: HCMC (High Conductive Magnesium Composite);Soft light start: No;Basic light level function: No;Main light adjustable: No;Interconnection: No;Output: 19,3 W;Colour Rendering Index CRI: = 82;Product category: LED floodlight without sensor;Energy efficiency class of light source: E

Manufacturer Steinel
Prod. No. 068097
Ordering designation XLED PRO 240 black

Deliver, install and set ready for operation
