**STEINEL Professional Bewegingsmelder**

**MD IR D180**

**COM1 - antraciet**

Dimensions (L x W x H): 42 x 116 x 116 mm; With motion detector: Ja; Manufacturer's Warranty: 5 jaar; Settings via: Smartphone, Tablet, Connect Bluetooth Mesh, App; With remote control: Nee; Version: COM1 - antraciet; PU1, EAN: 4007841066079; Type: Bewegingsmelder; Application, place: Buiten; Application, room: Buiten, tuin, entree, tuin & oprit, rondom het huis, terras / balkon, hal / gang, Binnen; Colour: antraciet; Colour, RAL: 7039; Includes corner wall mount: Nee; Installation site: wand; Installation: Op de muur, Wand; IP-rating: IP54; Ambient temperature: van -20 tot 40 °C; Materiaal: kunststof; Mains power supply: 220 – 240 V / 50 – 60 Hz; Switching output 1, resistive: 2000 W; Switching output 1, floating: Nee; Fluorescent lamps, electronic ballast: 500 W; Fluorescent lamps, uncorrected: 1000 VA; Fluorescent lamps, series-corrected: 400 VA; Fluorescent lamps, parallel-corrected: 400 VA; Switching output 1, low-voltage halogen lamps: 2000 VA; LED lamps < 2 W: 100 W; LED lamps > 2 W < 8 W: 250 W; LED lamps > 8 W: 500 W; Capacitive load in μF: 176 µF; Power consumption: 0,6 W; Technology, sensors: passief infrarood, Lichtsensor; Mounting height: 1,80 – 2,5 m; Mounting height max.: 2,50 m; Optimum mounting height: 2 m; Detection angle: 180 °; Angle of aperture: 90 °; Sneak-by guard: Ja; Capability of masking out individual segments: Ja; Electronic scalability: Ja; Mechanical scalability: Nee; Reach, radial: r = 6 m (57 m²); Reach, tangential: r = 9 m (127 m²); Functions: Bewegingssensor, Instelbare fade-tijd bij in- en uitschakelen, Definitie van het vangstgebied, Feedbackanzeige, Nachtspaarstand, Normaal- / testbedrijf, Buurgroepfunctie, Relaisuitgang, Lichtsensor; Twilight setting: 2 – 1000 lx; Time setting: 5 sec. – 60 min; Basic light level function: Nee; Main light adjustable: Nee; Twilight setting TEACH: Ja; Constant-lighting control: Nee; Interconnection: Ja; Interconnection via: Bluetooth Mesh; Product category: Bewegingsmelder

**Fabrikant** Steinel

**art.nr.** 066079

**Bestelaanduiding** MD IR D180 COM1 - antraciet

Leveren, monteren en bedrijfsklaar instellen