STEINEL Professional LED indoor light without sensor

RS PRO P1 flat
warm white

Dimensions (Ø x H): 272 x 64 mm;With lamp: Yes, STEINEL LED system;With motion detector: No;Manufacturer's Warranty: 5 years;Version: warm white;PU1, EAN: 4007841069704;Application, place: Indoors;Colour: white;Installation site: ceiling;Installation: Ceiling;Impact resistance: IK03;IP-rating: IP54;Protection class: II;Ambient temperature: from -10 up to 40 °C;Housing material: Plastic;Cover material: Plastic, opal;Mains power supply: 220 – 240 V / 50 – 60 Hz;Luminous flux total product: 922 lm;Total product efficiency: 112 lm/W;Colour temperature: 3000 K;Lamp: LED cannot be replaced;Base: without;LED cooling system: Passive Thermo Control;Soft light start: Yes;Main light adjustable: No;Interconnection via: Cable;Lifetime LED according to IEC-62717 (L70): 100.000 h;Lifetime LED according to IEC-62717 (L80): 73.000 h;LED service life according to IES TM-21 (L70): >60.000 h;Lifetime LED according to IES TM-21 (L80): >60.000 h;Fuse protection B10: 54;Fuse protection B16: 87;Fuse protection C10: 90;Fuse protection C16: 145;Output: 8,2 W;Colour Rendering Index CRI: = 82;Photobiological safety in accordance with EN 62471: RG1;Starting current, maximum: 13 A;IP-rating, ceiling: IP54;Product category: LED indoor light without sensor

Manufacturer Steinel
Prod. No. 069704
Ordering designation RS PRO P1 flat warm white

Deliver, install and set ready for operation
