**STEINEL Professional LED indoor light without sensor**

**RS PRO P2 flat**

**Neutral white**

Dimensions (Ø x H): 322 x 68 mm; With lamp: Yes, STEINEL LED system; With motion detector: No; Manufacturer's Warranty: 5 years; Version: Neutral white; PU1, EAN: 4007841069759; Colour: white; Installation site: wall, ceiling; Installation: Ceiling; Impact resistance: IK03; IP-rating: IP54; Protection class: II; Ambient temperature: from -10 up to 40 °C; Housing material: Plastic; Cover material: Plastic, opal; Mains power supply: 220 – 240 V / 50 – 60 Hz; Luminous flux total product: 1684 lm; Total product efficiency: 119 lm/W; Colour temperature: 4000 K; Lamp: LED cannot be replaced; Base: without; LED cooling system: Passive Thermo Control; Soft light start: Yes; Main light adjustable: No; Interconnection via: Cable; Lifetime LED according to IEC-62717 (L70): 100.000 h; Lifetime LED according to IEC-62717 (L80): 73.000 h; Lebensdauer LED nach IES TM-21 (L70): >60.000 h; Lifetime LED according to IES TM-21 (L80): >60.000 h; Fuse protection B10: 54; Fuse protection B16: 87; Fuse protection C10: 90; Fuse protection C16: 145; Output: 14,1 W; Colour Rendering Index CRI: = 82; Photobiological safety in accordance with EN 62471: RG1; Starting current, maximum: 13 A; IP-rating, ceiling: IP54; Product category: LED indoor light without sensor

**Manufacturer** Steinel

**Prod. No.** 069759

**Ordering designation** RS PRO P2 flat Neutral white

Deliver, install and set ready for operation