**STEINEL Professional Luminaire intérieur LED à détection**

**RS PRO LED P3 EM**

**Éclairage de secours - blanc neutre**

Dimensions (Ø x H): 400 x 142 mm; With lamp: Oui, système d'éclairage LED STEINEL; With motion detector: Oui; Manufacturer's Warranty: 5 ans; Version: Éclairage de secours - blanc neutre; PU1, EAN: 4007841058593; Colour: blanc; Installation site: mur, plafond; Installation: Plafond; Impact resistance: IK03; IP-rating: IP54; Protection class: II; Ambient temperature: de -10 jusqu'à 30 °C; Housing material: Matière plastique; Cover material: Matière plastique opale; Mains power supply: 220 – 240 V / 50 – 60 Hz; Mounting height max.: 4,00 m; Electronic scalability: Oui; Mechanical scalability: Non; Reach, radial: Ø 8 m (50 m²); Reach, tangential: Ø 8 m (50 m²); Luminous flux total product: 2188 lm; Total product efficiency: 123 lm/W; Colour temperature: 4000 K; Lamp: LED non interchangeable; Base: sans; LED cooling system: Contrôle thermique passif; Soft light start: Oui; Functions: Lumiére de secours selon la norme EN 60598-2-22 durant 3 heurres; Twilight setting: 2 – 2000 lx; Time setting: 5 s – 15 min; Basic light level function: Oui; Basic light level function time: 10/30 min, toute la nuit; Main light adjustable: Non; Interconnection: Oui; Interconnection via: Câble; Lifetime LED according to IEC-62717 (L70): 100.000 h; Lifetime LED according to IEC-62717 (L80): 74.000 h; Durée de vie des LED selon IES TM-21 (L70): >60.000 h; Lifetime LED according to IES TM-21 (L80): >60.000 h; Fuse protection B10: 54; Fuse protection B16: 87; Fuse protection C10: 90; Fuse protection C16: 145; Switching output 1, low-voltage halogen lamps: 800 VA; LED lamps > 8 W: 250 W; Capacitive load in μF: 88 µF; Basic light level function in per cent: 10 %; Output: 18,4 W; Colour Rendering Index CRI: = 82; Luminous flux, emergency light: 38 lm; Photobiological safety in accordance with EN 62471: RG1; Starting current, maximum: 13 A; IP-rating, ceiling: IP54; Detection angle: 360 °; Product category: Luminaire intérieur LED à détection

**Fabricant** Steinel

**Réf.** 058593

**Désignation commande** RS PRO LED P3 EM Éclairage de secours - blanc neutre

Livrer, monter et régler pour être opérationnel