**STEINEL Professional Lampada a sensore per interno LED**

**RS PRO LED P3 EM**

**Luce d'emergenza - Bianco neutro**

Dimensions (Ø x H): 400 x 142 mm; With lamp: Sì, sistema LED STEINEL; With motion detector: Sì; Manufacturer's Warranty: 5 anni; Version: Luce d'emergenza - Bianco neutro; PU1, EAN: 4007841058593; Colour: bianco; Installation site: Parete, soffitto; Installation: Soffitto; Impact resistance: IK03; IP-rating: IP54; Protection class: II; Ambient temperature: da -10 fino a 30 °C; Housing material: Plastica; Cover material: Plastica opalina; Mains power supply: 220 – 240 V / 50 – 60 Hz; Mounting height max.: 4,00 m; Electronic scalability: Sì; Mechanical scalability: No; Reach, radial: Ø 8 m (50 m²); Reach, tangential: Ø 8 m (50 m²); Luminous flux total product: 2188 lm; Total product efficiency: 123 lm/W; Colour temperature: 4000 K; Lamp: LED non sostituibile; Base: senza; LED cooling system: Passive Thermo Control; Soft light start: Sì; Functions: Luce di emergenza secondo la EN 60598-2-22 per 3 ore; Twilight setting: 2 – 2000 lx; Time setting: 5 sec – 15 min; Basic light level function: Sì; Basic light level function time: 10/30 min, tutta la notte; Main light adjustable: No; Interconnection: Sì; Interconnection via: Cavo; Lifetime LED according to IEC-62717 (L70): 100.000 h; Lifetime LED according to IEC-62717 (L80): 74.000 h; Durata dei LED secondo IES TM-21 (L70): >60.000 h; Lifetime LED according to IES TM-21 (L80): >60.000 h; Fuse protection B10: 54; Fuse protection B16: 87; Fuse protection C10: 90; Fuse protection C16: 145; Switching output 1, low-voltage halogen lamps: 800 VA; LED lamps > 8 W: 250 W; Capacitive load in μF: 88 µF; Basic light level function in per cent: 10 %; Output: 18,4 W; Colour Rendering Index CRI: = 82; Luminous flux, emergency light: 38 lm; Photobiological safety in accordance with EN 62471: RG1; Starting current, maximum: 13 A; IP-rating, ceiling: IP54; Detection angle: 360 °; Product category: Lampada a sensore per interno LED

**Produttore** Steinel

**Art. n.** 058593

**Denominazione ordine** RS PRO LED P3 EM Luce d'emergenza - Bianco neutro

Consegnare, montare e impostare in modo che sia pronto alla messa in funzione