**STEINEL Professional Sensor-LED-binnenlamp**

**RS PRO LED P3 EM**

**Noodverlichting - neutraal wit**

Dimensions (Ø x H): 400 x 142 mm; With lamp: Ja, STEINEL led-systeem; With motion detector: Ja; Manufacturer's Warranty: 5 jaar; Version: Noodverlichting - neutraal wit; PU1, EAN: 4007841058593; Colour: wit; Installation site: wand, plafond; Installation: Plafond; Impact resistance: IK03; IP-rating: IP54; Protection class: II; Ambient temperature: van -10 tot 30 °C; Housing material: kunststof; Cover material: Kunststof opaal; Mains power supply: 220 – 240 V / 50 – 60 Hz; Mounting height max.: 4,00 m; Electronic scalability: Ja; Mechanical scalability: Nee; Reach, radial: Ø 8 m (50 m²); Reach, tangential: Ø 8 m (50 m²); Luminous flux total product: 2188 lm; Total product efficiency: 123 lm/W; Colour temperature: 4000 K; Lamp: Led niet vervangbaar; Base: zonder; LED cooling system: Passive Thermo Control; Soft light start: Ja; Functions: Noodverlichtings conform EN 60598-2-22 gedurende 3 uur; Twilight setting: 2 – 2000 lx; Time setting: 5 sec. – 15 min; Basic light level function: Ja; Basic light level function time: 10/30 min., hele nacht; Main light adjustable: Nee; Interconnection: Ja; Interconnection via: Kabel; Lifetime LED according to IEC-62717 (L70): 100.000 h; Lifetime LED according to IEC-62717 (L80): 74.000 h; Levensduur LED volgens IES TM-21 (L70): >60.000 h; Lifetime LED according to IES TM-21 (L80): >60.000 h; Fuse protection B10: 54; Fuse protection B16: 87; Fuse protection C10: 90; Fuse protection C16: 145; Switching output 1, low-voltage halogen lamps: 800 VA; LED lamps > 8 W: 250 W; Capacitive load in μF: 88 µF; Basic light level function in per cent: 10 %; Output: 18,4 W; Colour Rendering Index CRI: = 82; Luminous flux, emergency light: 38 lm; Photobiological safety in accordance with EN 62471: RG1; Starting current, maximum: 13 A; IP-rating, ceiling: IP54; Detection angle: 360 °; Product category: Sensor-LED-binnenlamp

**Fabrikant** Steinel

**art.nr.** 058593

**Bestelaanduiding** RS PRO LED P3 EM Noodverlichting - neutraal wit

Leveren, monteren en bedrijfsklaar instellen