**STEINEL Professional Photoelectric lighting controller**

**TTS PRO**

**Anthracite**

Dimensions (L x W x H): 38 x 95 x 95 mm; With motion detector: No; Manufacturer's Warranty: 5 years; Settings via: Connect Bluetooth Mesh, App, Smartphone; With remote control: No; Version: Anthracite; PU1, EAN: 4007841089139; Type: Photo-cell controller; Application, place: Outdoors; Application, room: outdoors, front door, courtyard & driveway, Indoors, all round the building, terrace / balcony; Colour: Anthracite; Installation site: wall; Installation: Surface wiring, Wall; IP-rating: IP54; Ambient temperature: from -20 up to 40 °C; Material: Plastic; Mains power supply: 220 – 240 V / 50 – 60 Hz; Switching output 1, resistive: 1000 W; LED lamps > 8 W: 250 W; Power consumption: 0,5 W; Technology, sensors: Light sensor; Twilight setting: 1 – 1000 lx; Basic light level function: No; Twilight setting TEACH: Yes; Constant-lighting control: No; Interconnection: Yes; Type of interconnection: Master/master, Master/slave; Interconnection via: Bluetooth Mesh Connect; Product category: Photoelectric lighting controller

**Manufacturer** Steinel

**Prod. No.** 089139

**Ordering designation** TTS PRO Anthracite

Deliver, install and set ready for operation