**STEINEL Professional Sensor-switched LED indoor light**

**RS PRO R10 basic SC MP5**

**Neutral white**

Dimensions (Ø x H): 300 x 55 mm; With lamp: Yes, STEINEL LED system; Manufacturer's Warranty: 5 years; Settings via: Bluetooth; With remote control: No; Version: Neutral white; PU1, EAN: 4007841068424; Application, place: Indoors; Application, room: corridor / aisle, changing room, function room / ancillary room, kitchenette, stairwell, Indoors; includes sheet of self-adhesive numbers: No; Installation site: ceiling, wall; Impact resistance: IK07; IP-rating: IP40; Protection class: II; Ambient temperature: from -20 up to 40 °C; Housing material: Plastic; Cover material: PC, opal; Mains power supply: 220 – 240 V / 50 – 60 Hz; Power consumption: 0,3 W; HF-system: 5,8 GHz; Slave modeselectable: Yes; Lamp: LED cannot be replaced; Base: without; LED cooling system: Passive Thermo Control; Continuous light: selectable; Functions: Group parameterisation, Manual ON / ON-OFF, Neighbouring group function, Orientation light, Motions sensor, Light sensor, Encrypted communication, Free selection of the light value in a luminaire group, Adjustable fade time when switching on and off; Time setting: 5 sec – 60 min; Basic light level function: Yes; Basic light level function time: 1-60 min; Main light adjustable: 0 - 100 %; Interconnection: Yes; Type of interconnection: Master/master; Interconnection via: Bluetooth Mesh; Lifetime LED according to IEC-62717 (L70): 100.000 h; Lifetime LED according to IEC-62717 (L80): 74.000 h; Lebensdauer LED nach IES TM-21 (L70): >60.000 h; Lifetime LED according to IES TM-21 (L80): >60.000 h; Fuse protection B10: 46; Fuse protection B16: 74; Fuse protection C10: 77; Fuse protection C16: 122; Basic light level function in per cent: 0 – 100 %; Photobiological safety in accordance with EN 62471: RG1; Starting current, maximum: 13 A; IP-rating, ceiling: IP40; Product category: Sensor-switched LED indoor light

**Manufacturer** Steinel

**Prod. No.** 068424

**Ordering designation** RS PRO R10 basic SC MP5 Neutral white

Deliver, install and set ready for operation