STEINEL Professional Light sensor

TCL PRO
white

Dimensions (L x W x H): 38 x 95 x 95 mm;With motion detector: No;Manufacturer's Warranty: 5 years;Settings via: Bluetooth Mesh, App, Smartphone;With remote control: No;Version: white;PU1, EAN: 4007841089146;Type: Photo-cell controller;Application, place: Outdoors;Application, room: outdoors, front door, courtyard & driveway, Indoors, all round the building, terrace / balcony;Colour: white;Colour, RAL: 9003;Installation site: wall;Installation: Surface wiring, Wall;IP-rating: IP54;Ambient temperature: from -20 up to 40 °C;Material: Plastic;Mains power supply: 220 – 240 V / 50 – 60 Hz;Power consumption: 0,5 W;Technology, sensors: Other;Mounting height: 1,80 – 4,00 m;Mounting height max.: 4,00 m;Optimum mounting height: 2 m;Twilight setting: 1 – 1000 lx;Basic light level function: No;Twilight setting TEACH: Yes;Constant-lighting control: No;Interconnection: Yes;Type of interconnection: Master/master, Master/slave;Interconnection via: Bluetooth Mesh;Product category: Light sensor

Manufacturer Steinel
Prod. No. 089146
Ordering designation TCL PRO white

Deliver, install and set ready for operation
