**STEINEL Professional Motion detector**

**MD IR N130**

**COM1 - surface white**

Dimensions (L x W x H): 87 x 82 x 98 mm; With motion detector: Yes; Manufacturer's Warranty: 5 years; Settings via: Bluetooth, Smartphone, Tablet; With remote control: No; Version: COM1 - surface white; PU1, EAN: 4007841069056; Type: Motion detectors; Application, place: Outdoors, Indoors; Application, room: front door, all round the building, terrace / balcony, outdoors, courtyard & driveway, Indoors; Colour: white; Includes corner wall mount: No; Installation site: corner, wall; Installation: Surface wiring; IP-rating: IP54; Protection class: II; Ambient temperature: from -20 up to 40 °C; Material: Plastic; Mains power supply: 220 – 240 V / 50 – 60 Hz; Switching output 1, resistive: 2000 W; Switching output 1, number of LEDs / fluorescent lamps: 10 pcs.; Power consumption: 0,5 W; Technology, sensors: passive infrared, Light sensor; Mounting height: 1,80 – 4,00 m; Mounting height max.: 4,00 m; Optimum mounting height: 2 m; Detection angle: 130 °; Sneak-by guard: Yes; Capability of masking out individual segments: Yes; Electronic scalability: Yes; Mechanical scalability: Yes; Reach, radial: r = 2.5 m (7 m²); Reach, tangential: r = 13 m (192 m²); Cover material: shrouds; Functions: Motions sensor, Light sensor, Relay output, Data monitoring; Twilight setting: 2 – 2000 lx; Time setting: 5 sec – 60 min; Basic light level function: No; Twilight setting TEACH: Yes; Constant-lighting control: No; Interconnection: Yes; Interconnection via: Bluetooth Mesh; Reichweite Radial Eagle Eye max.: 6 m; Product category: Motion detector

**Manufacturer** Steinel

**Prod. No.** 069056

**Ordering designation** MD IR N130 COM1 - surface white

Deliver, install and set ready for operation