**STEINEL Professional Sensore di movimento**

**MD IR N270**

**COM1 - sup. bianco**

Dimensions (L x W x H): 87 x 82 x 98 mm; With motion detector: Sì; Manufacturer's Warranty: 5 anni; Settings via: Bluetooth, Smartphone, Tablet; With remote control: No; Version: COM1 - sup. bianco; PU1, EAN: 4007841079819; Type: Rilevatori di movimento; Application, place: Esterno, Interni; Application, room: terrazzi / balconi, perimetro della casa, parcheggi coperti / garage sotterranei, Cortili e passi carrai, Esterno, Interni, ingressi di abitazioni; Colour: bianco; Includes corner wall mount: Sì; Installation site: angolo, Parete; Installation: In superficie; IP-rating: IP54; Protection class: II; Ambient temperature: da -20 fino a 40 °C; Materiale: Plastica; Mains power supply: 220 – 240 V / 50 – 60 Hz; Switching output 1, resistive: 2000 W; Switching output 1, number of LEDs / fluorescent lamps: 10 pz; Power consumption: 0,3 W; Technology, sensors: Infrarossi passivi, Sensore ottico; Mounting height: 1,80 – 6,00 m; Mounting height max.: 6,00 m; Optimum mounting height: 2 m; Detection angle: 270 °; Sneak-by guard: Sì; Capability of masking out individual segments: Sì; Electronic scalability: Sì; Mechanical scalability: No; Reach, radial: r = 2.7 m (17 m²); Reach, tangential: r = 12.5 m (368 m²); Cover material: calotte di copertura; Functions: Sensore di luce, Sensore di movimento, Uscita a relè, Monitoraggio dei dati; Twilight setting: 2 – 2000 lx; Time setting: 5 sec – 60 min; Basic light level function: No; Main light adjustable: No; Twilight setting TEACH: Sì; Constant-lighting control: No; Interconnection: Sì; Interconnection via: Bluetooth; Reichweite Radial Eagle Eye max.: 6 m; Product category: Sensore di movimento

**Produttore** Steinel

**Art. n.** 079819

**Denominazione ordine** MD IR N270 COM1 - sup. bianco

Consegnare, montare e impostare in modo che sia pronto alla messa in funzione